(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FFC_Amphenol_1x40_62684-401100AHLF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 21.59 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FFC_Amphenol_1x40_62684-401100AHLF"
				(at 21.59 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FFC_Amphenol_1x40_62684-401100AHLF"
				(at 21.59 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/62684.pdf"
				(at 21.59 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FFC & FPC Connectors, 40 pin, 0.5mm, SMD/SMT, Right Angle, Bottom Concact"
				(at 21.59 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "62684-401100AHLF"
				(at 21.59 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 21.59 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 21.59 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 21.59 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, FFC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FFC_Amphenol_1x40_62684-401100AHLF_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 2.54)
					(name "")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 2.54)
					(name "")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 2.54)
					(name "")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
