(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PinHeader_2x17_P1.27mm_SMD_Shrouded"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 25.4 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PinHeader_2x17_P1.27mm_SMD_Shrouded"
				(at 25.4 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PinHeader_2x17_P1.27mm_SMD_Shrouded"
				(at 25.4 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/catalog/datasheet/62703420621.pdf"
				(at 25.4 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pin Header, Wire-to-Board, 1.27 mm, 2 Rows, 34 Contacts, Surface Mount Straight, WR-BHD Series"
				(at 25.4 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "62703420621"
				(at 25.4 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 25.4 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "PINSTRIP, HEADER, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PinHeader_2x17_P1.27mm_SMD_Shrouded_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 10.16 -10.16 180)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin passive line
					(at 10.16 -12.7 180)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 10.16 -15.24 180)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 10.16 -17.78 180)
					(length 2.54)
					(name "")
					(number "16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "")
					(number "17")
				)
				(pin passive line
					(at 10.16 -20.32 180)
					(length 2.54)
					(name "")
					(number "18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "")
					(number "19")
				)
				(pin passive line
					(at 10.16 -22.86 180)
					(length 2.54)
					(name "")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "")
					(number "21")
				)
				(pin passive line
					(at 10.16 -25.4 180)
					(length 2.54)
					(name "")
					(number "22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "")
					(number "23")
				)
				(pin passive line
					(at 10.16 -27.94 180)
					(length 2.54)
					(name "")
					(number "24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "")
					(number "25")
				)
				(pin passive line
					(at 10.16 -30.48 180)
					(length 2.54)
					(name "")
					(number "26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "")
					(number "27")
				)
				(pin passive line
					(at 10.16 -33.02 180)
					(length 2.54)
					(name "")
					(number "28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "")
					(number "29")
				)
				(pin passive line
					(at 10.16 -35.56 180)
					(length 2.54)
					(name "")
					(number "30")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "")
					(number "31")
				)
				(pin passive line
					(at 10.16 -38.1 180)
					(length 2.54)
					(name "")
					(number "32")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "")
					(number "33")
				)
				(pin passive line
					(at 10.16 -40.64 180)
					(length 2.54)
					(name "")
					(number "34")
				)
			)
			(embedded_fonts no)
		)
)
