(footprint "USB-Micro-B_Receptacle_WE_629105150521"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "USB Micro-B receptacle")
	(tags "usb micro receptacle")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-Micro-B_Receptacle_WE_629105150521"
		(at 0 4.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.151 6.551 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.151 7.55 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.151 8.55 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at -2.5 -1.849)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole oval
		(at 2.499 -1.849)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.301 -2.949)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.652 -2.949)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0 -2.949)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.65 -2.949)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 1.3 -2.949)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" thru_hole oval
		(at -3.875 0.901)
		(size 1.15 1.8)
		(drill oval 0.55 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -3.726 -2.899)
		(size 1.45 2)
		(drill oval 0.85 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.725 -2.899)
		(size 1.45 2)
		(drill oval 0.85 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.874 0.901)
		(size 1.15 1.8)
		(drill oval 0.55 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_629105150521.glb"
		(offset
			(xyz 0 2.048435 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
