(footprint "USB-Micro-B_Receptacle_WE_629105150921"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "USB - micro B, USB 2.0, Connector, 5 Position Surface Mount, Right Angle; Through Hole ")
	(tags "USB micro B, 2.0, connector")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-Micro-B_Receptacle_WE_629105150921"
		(at 0 3.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.1 6.11 0)
		(layer "F.Fab")
	)
	(fp_text user "PCB Edge"
		(at -5.1 7.31 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.1 8.51 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.1 9.71 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.301 -2.806)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.652 -2.806)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -2.806)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -2.806 180)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -2.806 180)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -4.175 0)
		(size 2.25 1.9)
		(drill oval 0.75 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.26 -3.121)
		(size 1.15 1.05)
		(drill oval 0.75 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" smd rect
		(at -1.15 0)
		(size 1.8 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 1.148 0)
		(size 1.8 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at 2.258 -3.121)
		(size 1.15 1.05)
		(drill oval 0.75 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.174 0)
		(size 2.25 1.9)
		(drill oval 0.75 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_629105150921.glb"
		(offset
			(xyz 0 2 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
