(footprint "USB-C_Receptacle_WE_632723300011"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.001 -7.398 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-C_Receptacle_WE_632723300011"
		(at 0.001 7.402 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "PCB edge"
		(at -2.539 4.772 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.271 8.497 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.271 9.697 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.271 10.897 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0 -1.055)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 2.045)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A1" smd roundrect
		(at -2.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A2" smd roundrect
		(at -2.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A3" smd roundrect
		(at -1.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A4" smd roundrect
		(at -1.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A5" smd roundrect
		(at -0.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A6" smd roundrect
		(at -0.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A7" smd roundrect
		(at 0.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A8" smd roundrect
		(at 0.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A9" smd roundrect
		(at 1.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A10" smd roundrect
		(at 1.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A11" smd roundrect
		(at 2.25 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A12" smd roundrect
		(at 2.75 -5.635)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B1" thru_hole circle
		(at 2.8 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B2" thru_hole circle
		(at 2.4 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B3" thru_hole circle
		(at 1.6 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at 1.2 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at 0.8 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at 0.4 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at -0.4 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at -0.8 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at -1.2 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B10" thru_hole circle
		(at -1.6 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B11" thru_hole circle
		(at -2.4 -3.685)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at -2.8 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.27 -3.235)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.27 1.495)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -2 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 2 -4.385)
		(size 0.65 0.65)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.27 -3.235)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.27 1.495)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_632723300011.glb"
		(offset
			(xyz 0.001 -0.002 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
