(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCIe_x4_Molex_67910-5700"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCIe_x4_Molex_67910-5700"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCIe_x4_Molex_67910-5700"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheet.datasheetarchive.com/originals/distributors/Datasheets_SAMA/50bcc70a7102e69944e39fc33a0bf013.pdf"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PCI Express/0.8MM PITCH MINI PCI TCH MINI PCI-E CONN."
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "67910-5700"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, PCIE, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCIe_x4_Molex_67910-5700_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 13.97 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 13.97 -2.54 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 13.97 -5.08 180)
					(length 2.54)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at 13.97 -7.62 180)
					(length 2.54)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "9")
					(number "9")
				)
				(pin passive line
					(at 13.97 -10.16 180)
					(length 2.54)
					(name "10")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "11")
					(number "11")
				)
				(pin passive line
					(at 13.97 -12.7 180)
					(length 2.54)
					(name "12")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "13")
					(number "13")
				)
				(pin passive line
					(at 13.97 -15.24 180)
					(length 2.54)
					(name "14")
					(number "14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "15")
					(number "15")
				)
				(pin passive line
					(at 13.97 -17.78 180)
					(length 2.54)
					(name "16")
					(number "16")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "17")
					(number "17")
				)
				(pin passive line
					(at 13.97 -22.86 180)
					(length 2.54)
					(name "18")
					(number "18")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "19")
					(number "19")
				)
				(pin passive line
					(at 13.97 -25.4 180)
					(length 2.54)
					(name "20")
					(number "20")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "21")
					(number "21")
				)
				(pin passive line
					(at 13.97 -27.94 180)
					(length 2.54)
					(name "22")
					(number "22")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "23")
					(number "23")
				)
				(pin passive line
					(at 13.97 -30.48 180)
					(length 2.54)
					(name "24")
					(number "24")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "25")
					(number "25")
				)
				(pin passive line
					(at 13.97 -33.02 180)
					(length 2.54)
					(name "26")
					(number "26")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "27")
					(number "27")
				)
				(pin passive line
					(at 13.97 -35.56 180)
					(length 2.54)
					(name "28")
					(number "28")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "29")
					(number "29")
				)
				(pin passive line
					(at 13.97 -38.1 180)
					(length 2.54)
					(name "30")
					(number "30")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "31")
					(number "31")
				)
				(pin passive line
					(at 13.97 -40.64 180)
					(length 2.54)
					(name "32")
					(number "32")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "33")
					(number "33")
				)
				(pin passive line
					(at 13.97 -43.18 180)
					(length 2.54)
					(name "34")
					(number "34")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "35")
					(number "35")
				)
				(pin passive line
					(at 13.97 -45.72 180)
					(length 2.54)
					(name "36")
					(number "36")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "37")
					(number "37")
				)
				(pin passive line
					(at 13.97 -48.26 180)
					(length 2.54)
					(name "38")
					(number "38")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "39")
					(number "39")
				)
				(pin passive line
					(at 13.97 -50.8 180)
					(length 2.54)
					(name "40")
					(number "40")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "41")
					(number "41")
				)
				(pin passive line
					(at 13.97 -53.34 180)
					(length 2.54)
					(name "42")
					(number "42")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "43")
					(number "43")
				)
				(pin passive line
					(at 13.97 -55.88 180)
					(length 2.54)
					(name "44")
					(number "44")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "45")
					(number "45")
				)
				(pin passive line
					(at 13.97 -58.42 180)
					(length 2.54)
					(name "46")
					(number "46")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "47")
					(number "47")
				)
				(pin passive line
					(at 13.97 -60.96 180)
					(length 2.54)
					(name "48")
					(number "48")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "49")
					(number "49")
				)
				(pin passive line
					(at 13.97 -63.5 180)
					(length 2.54)
					(name "50")
					(number "50")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "51")
					(number "51")
				)
				(pin passive line
					(at 13.97 -66.04 180)
					(length 2.54)
					(name "52")
					(number "52")
				)
				(pin passive line
					(at 13.97 -71.12 180)
					(length 2.54)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
