(footprint "HDMI-Mini-C_Receptacle_WE_685119136923"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.249 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI-Mini-C_Receptacle_WE_685119136923"
		(at 0 5.251 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -6.125 11.14 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -6.125 12.34 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.125 13.54 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 3.6 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.2 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.798 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.398 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.999 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.6 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.199 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.8 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.4 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.402 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -0.802 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.2 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.601 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -2 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -2.4 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -2.801 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.202 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.601 -3.4)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -5.425 -2.35)
		(size 1.2 1.9)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -5.425 2.15)
		(size 1.2 1.7)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 5.424 -2.35)
		(size 1.2 1.9)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 5.424 2.15)
		(size 1.2 1.7)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_685119136923.glb"
		(offset
			(xyz 0 2.35 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
