(footprint "WE_68712414022"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "<b>WR-FPC 0.5mm SMT ZIF Horizontal Top Contact, 24 Pins")
	(property "Reference" "REF**"
		(at 6.28 -2.226 0)
		(layer "F.SilkS")
	)
	(property "Value" "WE_68712414022"
		(at 8.89 5.97 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "1"
		(at -0.855 -1.442 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -4.451 7.97 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.451 9.17 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.451 10.371 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.498 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.998 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.498 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.998 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 5.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 5.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 6.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 6.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 7.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 7.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 8.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 8.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 9.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 9.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 10.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 10.999 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 11.499 0)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Z1" smd rect
		(at -1.93 1.86)
		(size 2.7 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Z2" smd rect
		(at 13.428 1.86)
		(size 2.7 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_68712414022.glb"
		(offset
			(xyz 5.75 -1.86 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 180 180)
		)
	)
)
