(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WE_68712414022"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WE_68712414022"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WE_68712414022"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/components/products/datasheet/68712414022.pdf"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FFC / FPC Board Connector, Right Angle, 0.5 mm, 24 Contacts, Receptacle, Surface Mount, Top"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "68712414022"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WE_68712414022_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "Pin_8")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "Pin_9")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "Pin_10")
					(number "10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "Pin_11")
					(number "11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "Pin_12")
					(number "12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "Pin_13")
					(number "13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "Pin_14")
					(number "14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "Pin_15")
					(number "15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "Pin_16")
					(number "16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "Pin_17")
					(number "17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "Pin_18")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "Pin_19")
					(number "19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "Pin_20")
					(number "20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "Pin_21")
					(number "21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "Pin_22")
					(number "22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "Pin_23")
					(number "23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "Pin_24")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
