(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCIe_x4_Conn_EdgeMount_NoMilling"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCIe_x4_Conn_EdgeMount_NoMilling"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCIe_x4_Conn_EdgeMount_NoMilling"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734857%7FC%7Fpdf%7FEnglish%7FENG_CD_1734857_C.pdf%7F6-1734857-5"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "64 Position Female Connector PCI Express™ Gold 0.039\" (1.00mm) Black"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "6-1734857-5"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCIe_x4_Conn_EdgeMount_NoMilling_0_1")
			(symbol "PCIe_x4_Conn_EdgeMount_NoMilling_1_1"
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(name "PRSNT#1")
					(number "A1")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "+12V")
					(number "A2")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "+12V")
					(number "A3")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "JTAG2")
					(number "A5")
				)
				(pin passive line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "JTAG3")
					(number "A6")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "JTAG4")
					(number "A7")
				)
				(pin passive line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "JTAG5")
					(number "A8")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "+3V3")
					(number "A9")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "+3V3")
					(number "A10")
				)
				(pin passive line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "PWRGD")
					(number "A11")
				)
				(pin passive line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 33.02 -33.02 180)
					(length 3.81)
					(name "REFCLK+")
					(number "A13")
				)
				(pin passive line
					(at 33.02 -35.56 180)
					(length 3.81)
					(name "REFCLK-")
					(number "A14")
				)
				(pin passive line
					(at 33.02 -38.1 180)
					(length 3.81)
					(name "GND")
					(number "A15")
				)
				(pin passive line
					(at 33.02 -40.64 180)
					(length 3.81)
					(name "HSIp(0)")
					(number "A16")
				)
				(pin passive line
					(at 33.02 -43.18 180)
					(length 3.81)
					(name "HSIn(0)")
					(number "A17")
				)
				(pin passive line
					(at 33.02 -45.72 180)
					(length 3.81)
					(name "GND")
					(number "A18")
				)
				(pin passive line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "RSVD")
					(number "A19")
				)
				(pin passive line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "GND")
					(number "A20")
				)
				(pin passive line
					(at 33.02 -53.34 180)
					(length 3.81)
					(name "HSIp(1)")
					(number "A21")
				)
				(pin passive line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "HSIn(1)")
					(number "A22")
				)
				(pin passive line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "GND")
					(number "A23")
				)
				(pin passive line
					(at 33.02 -60.96 180)
					(length 3.81)
					(name "GND")
					(number "A24")
				)
				(pin passive line
					(at 33.02 -63.5 180)
					(length 3.81)
					(name "HSIp(2)")
					(number "A25")
				)
				(pin passive line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "HSIn(2)")
					(number "A26")
				)
				(pin passive line
					(at 33.02 -68.58 180)
					(length 3.81)
					(name "GND")
					(number "A27")
				)
				(pin input line
					(at 33.02 -71.12 180)
					(length 3.81)
					(name "GND")
					(number "A28")
				)
				(pin passive line
					(at 33.02 -73.66 180)
					(length 3.81)
					(name "HSIp(3)")
					(number "A29")
				)
				(pin passive line
					(at 33.02 -76.2 180)
					(length 3.81)
					(name "HSIn(3)")
					(number "A30")
				)
				(pin passive line
					(at 33.02 -78.74 180)
					(length 3.81)
					(name "GND")
					(number "A31")
				)
				(pin passive line
					(at 33.02 -81.28 180)
					(length 3.81)
					(name "RSVD")
					(number "A32")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "+12V")
					(number "B1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "+12V")
					(number "B2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "+12V")
					(number "B3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SMCLK")
					(number "B5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SMDAT")
					(number "B6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "+3V3")
					(number "B8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "JTAG1")
					(number "B9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "+3V3aux")
					(number "B10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "WAKE#")
					(number "B11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "RSVD")
					(number "B12")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "HSOp(0)")
					(number "B14")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "HSOn(0)")
					(number "B15")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "GND")
					(number "B16")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PRSNT#2")
					(number "B17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "GND")
					(number "B18")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "HSOp(1)")
					(number "B19")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "HSOn(1)")
					(number "B20")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GND")
					(number "B21")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "HSOp(2)")
					(number "B23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "HSOn(2)")
					(number "B24")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "GND")
					(number "B25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "B26")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "HSOp(3)")
					(number "B27")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "HSOn(3)")
					(number "B28")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "GND")
					(number "B29")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "RSVD")
					(number "B30")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PRSNT#2")
					(number "B31")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "GND")
					(number "B32")
				)
			)
			(embedded_fonts no)
		)
)
