(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DVI-I_Molex_74320-9010"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DVI-I_Molex_74320-9010"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DVI-I_Molex_74320-9010"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.molex.com/pdm_docs/sd/743209010_sd.pdf"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DVI Connector, DVI-I (Integrated), Right Angle, Through Hole, Receptacle, 29 Contacts, Panel Mount"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74320-9010"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DVI-I_Molex_74320-9010_0_1")
			(symbol "DVI-I_Molex_74320-9010_1_1"
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D2-")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D2+")
					(number "2")
				)
				(pin power_in line
					(at 0 -63.5 0)
					(length 2.54)
					(name "D2/4_SH")
					(number "3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "D4-")
					(number "4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "D4+")
					(number "5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "DDC_CLK")
					(number "6")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "DDC_DATA")
					(number "7")
				)
				(pin passive line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "VERT_SYNC")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D1-")
					(number "9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D1+")
					(number "10")
				)
				(pin power_in line
					(at 0 -66.04 0)
					(length 2.54)
					(name "D1/3_SH")
					(number "11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "D3-")
					(number "12")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D3+")
					(number "13")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_in line
					(at 25.4 -66.04 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin passive line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "HP_DET")
					(number "16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "D0-")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "D0+")
					(number "18")
				)
				(pin power_in line
					(at 0 -68.58 0)
					(length 2.54)
					(name "D0/5_SH")
					(number "19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "D5-")
					(number "20")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "D5+")
					(number "21")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 2.54)
					(name "CLK_SH")
					(number "22")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "CLK+")
					(number "23")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "CLK-")
					(number "24")
				)
				(pin passive line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "A_RED")
					(number "C1")
				)
				(pin passive line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "A_GREEN")
					(number "C2")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "A_BLUE")
					(number "C3")
				)
				(pin passive line
					(at 25.4 -48.26 180)
					(length 2.54)
					(name "HORIZ_SYNC")
					(number "C4")
				)
				(pin power_in line
					(at 25.4 -63.5 180)
					(length 2.54)
					(name "A_GND")
					(number "C5")
				)
				(pin power_in line
					(at 25.4 -68.58 180)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
