(footprint "PCIe_x8_Guide_74540-0201"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -21 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "PCIe_x8_Guide_74540-0201"
		(at 0 21.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -23.45 24.595 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -23.45 25.795 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -23.45 26.995 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -18.26 -5.695)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.127)
	)
	(pad "" np_thru_hole circle
		(at 18.26 -5.695)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.127)
	)
	(pad "MP" thru_hole circle
		(at -18.75 -11.695)
		(size 3.175 3.175)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at -18.75 3.305)
		(size 3.175 3.175)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 18.75 -11.695)
		(size 3.175 3.175)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 18.75 3.305)
		(size 3.175 3.175)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" smd custom
		(at -20.215 10.105)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -29.48) (xy 7.265 -29.48) (xy 7.265 -27.37) (xy 2.695 -27.37) (xy 2.695 -3.3) (xy 37.735 -3.3)
					(xy 37.735 -27.37) (xy 32.765 -27.37) (xy 32.765 -29.48) (xy 40.43 -29.48) (xy 40.43 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "SH" smd rect
		(at -11 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -8.6 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.2 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd custom
		(at -4.25 -19.375)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 2.10999) (xy 8.1 2.10999) (xy 8.1 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "SH" smd rect
		(at 5.8 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 8.2 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 10.6 -18.32)
		(size 0.9 2.11)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_74540_0201.glb"
		(offset
			(xyz 0 -19.385 3.7)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
