(footprint "MP_Terminal_M4_THT_7461111"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -5.5 -5.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MP_Terminal_M4_THT_7461111"
		(at -5.41 6.51 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(attr through_hole allow_soldermask_bridges)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -5.41 7.71 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.41 8.91 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.41 10.11 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "1" thru_hole circle
		(at -3.81 -3.81)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -3.81 -1.27 270)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -3.81 1.27 90)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -3.81 3.81)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1.27 -3.81 180)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1.27 -1.27)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1.27 1.27)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1.27 3.81 180)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1.27 -3.81)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1.27 -1.27 180)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1.27 1.27 90)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1.27 3.81)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 -3.81 180)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 -1.27 270)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 1.27 90)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 3.81 180)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_7461111.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
