(footprint "Bus_RJ45_7498111120R"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -12 0)
		(layer "F.SilkS")
	)
	(property "Value" "Bus_RJ45_7498111120R"
		(at -9.7 13.525 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Recommended board cutout"
		(at -7.55 2.2 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.875 15.8 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.875 17 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -9.875 18.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.5 6.96)
		(size 2.1 2.1)
		(drill 1.4)
	)
	(pad "" np_thru_hole circle
		(at 0 -4.22)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.5 6.96)
		(size 2.1 2.1)
		(drill 1.4)
	)
	(pad "1" smd roundrect
		(at -6.605 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -5.59 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.57 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.555 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.54 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.525 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.51 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.51 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.525 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 2.54 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 3.555 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 4.57 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 5.59 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 6.605 11.1)
		(size 0.71 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at -8.6 -3.24)
		(size 1.2 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at 8.6 -3.24)
		(size 1.2 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_7498111120r.glb"
		(offset
			(xyz 0 11.239 3.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
)
