(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_RJ45_7498111120R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 41.91 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_RJ45_7498111120R"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_RJ45_7498111120R"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/407/7498111120R.pdf"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular Connector, RJ45 Jack, 1 x 1 (Port), Surface Mount"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "7498111120R"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RJ45, HORIZONTAL, SMT, ETHERNET, CONNECTOR, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_RJ45_7498111120R_1_1"
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "LED2_G-")
					(number "1")
				)
				(pin passive line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "LED2_G+")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D1+")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D1-")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D2+")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D2-")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D3+")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D3-")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D4+")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D4-")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "11")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "LED1_Y-")
					(number "13")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(name "LED1_Y+")
					(number "14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
