(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PinHeader_2x26_P2.54mm_Drill1.1mm"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PinHeader_2x26_P2.54mm_Drill1.1mm"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PinHeader_2x26_P2.54mm_Drill1.1mm"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/documentation/datasheet/boardwiretoboard/bwb_bergstik.pdf"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pin Header, Vertical, Board-to-Board, 2.54 mm, 2 Rows, 52 Contacts, Through Hole Straight"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "77313-127-52LF"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HEADER, CONNECTOR, THT, MALE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PinHeader_2x26_P2.54mm_Drill1.1mm_1_1"
				(text ""
					(at 2.54 -40.64 0)
				)
				(text ""
					(at 2.54 -40.64 0)
				)
				(text ""
					(at 2.54 -43.18 0)
				)
				(text ""
					(at 2.54 -48.26 0)
				)
				(text ""
					(at 2.54 -50.8 0)
				)
				(text ""
					(at 2.54 -53.34 0)
				)
				(text ""
					(at 2.54 -55.88 0)
				)
				(text ""
					(at 2.54 -58.42 0)
				)
				(text ""
					(at 2.54 -60.96 0)
				)
				(text ""
					(at 2.54 -63.5 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 10.16 -10.16 180)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin passive line
					(at 10.16 -12.7 180)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 10.16 -15.24 180)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 10.16 -17.78 180)
					(length 2.54)
					(name "")
					(number "16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "")
					(number "17")
				)
				(pin passive line
					(at 10.16 -20.32 180)
					(length 2.54)
					(name "")
					(number "18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "")
					(number "19")
				)
				(pin passive line
					(at 10.16 -22.86 180)
					(length 2.54)
					(name "")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "")
					(number "21")
				)
				(pin passive line
					(at 10.16 -25.4 180)
					(length 2.54)
					(name "")
					(number "22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "")
					(number "23")
				)
				(pin passive line
					(at 10.16 -27.94 180)
					(length 2.54)
					(name "")
					(number "24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "")
					(number "25")
				)
				(pin passive line
					(at 10.16 -30.48 180)
					(length 2.54)
					(name "")
					(number "26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "")
					(number "27")
				)
				(pin passive line
					(at 10.16 -33.02 180)
					(length 2.54)
					(name "")
					(number "28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "")
					(number "29")
				)
				(pin passive line
					(at 10.16 -35.56 180)
					(length 2.54)
					(name "")
					(number "30")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "")
					(number "31")
				)
				(pin passive line
					(at 10.16 -38.1 180)
					(length 2.54)
					(name "")
					(number "32")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "")
					(number "33")
				)
				(pin passive line
					(at 10.16 -40.64 180)
					(length 2.54)
					(name "")
					(number "34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "")
					(number "35")
				)
				(pin passive line
					(at 10.16 -43.18 180)
					(length 2.54)
					(name "")
					(number "36")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "")
					(number "37")
				)
				(pin passive line
					(at 10.16 -45.72 180)
					(length 2.54)
					(name "")
					(number "38")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "")
					(number "39")
				)
				(pin passive line
					(at 10.16 -48.26 180)
					(length 2.54)
					(name "")
					(number "40")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "")
					(number "41")
				)
				(pin passive line
					(at 10.16 -50.8 180)
					(length 2.54)
					(name "")
					(number "42")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "")
					(number "43")
				)
				(pin passive line
					(at 10.16 -53.34 180)
					(length 2.54)
					(name "")
					(number "44")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "")
					(number "45")
				)
				(pin passive line
					(at 10.16 -55.88 180)
					(length 2.54)
					(name "")
					(number "46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "")
					(number "47")
				)
				(pin passive line
					(at 10.16 -58.42 180)
					(length 2.54)
					(name "")
					(number "48")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "")
					(number "49")
				)
				(pin passive line
					(at 10.16 -60.96 180)
					(length 2.54)
					(name "")
					(number "50")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "")
					(number "51")
				)
				(pin passive line
					(at 10.16 -63.5 180)
					(length 2.54)
					(name "")
					(number "52")
				)
			)
			(embedded_fonts no)
		)
)
