(footprint "Conn_FFC_8-188275-2"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -8.215 -4.35 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_FFC_8-188275-2"
		(at -8.39 4.95 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -2 4.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2 5.7 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.85 -6.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.365 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.097 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.825 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.556 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.285 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.016 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.255 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.525 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.795 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 5.064 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.334 -2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 7.605 2.25)
		(size 1.5 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_8_188275_2.glb"
		(offset
			(xyz 0.6 0 5.25)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
