(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "arty_chipKIT_connector"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 33.02 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "arty_chipKIT_connector"
				(at 33.02 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "arty_chipKIT_connector"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://digilent.com/reference/programmable-logic/arty-a7/reference-manual"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Connector Header Through Hole 40 position 0.100\" (2.54mm)"
				(at 33.02 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "9-146281-0"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer1" "TE Conectivity"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN1" "2-826629-0"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer2" "HARWIN"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN2" "M20-7830346"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "VERTICAL, THT, HEADER, CONNECTOR, MALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "arty_chipKIT_connector_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "NC")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IOREF")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RST")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "3V3")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "5V")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VIN")
					(number "8")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A0")
					(number "9")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A1")
					(number "10")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A2")
					(number "11")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A3")
					(number "12")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A4")
					(number "13")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A5")
					(number "14")
				)
				(pin input line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "V_P")
					(number "15")
				)
				(pin input line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "V_N")
					(number "16")
				)
				(pin input line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "XGND")
					(number "17")
				)
				(pin input line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "XVREF")
					(number "18")
				)
				(pin input line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "A6")
					(number "19")
				)
				(pin input line
					(at 17.78 -25.4 180)
					(length 2.54)
					(name "A7")
					(number "20")
				)
				(pin input line
					(at 17.78 -27.94 180)
					(length 2.54)
					(name "A8")
					(number "21")
				)
				(pin input line
					(at 17.78 -30.48 180)
					(length 2.54)
					(name "A9")
					(number "22")
				)
				(pin input line
					(at 17.78 -33.02 180)
					(length 2.54)
					(name "A10")
					(number "23")
				)
				(pin input line
					(at 17.78 -35.56 180)
					(length 2.54)
					(name "A11")
					(number "24")
				)
			)
			(symbol "arty_chipKIT_connector_2_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "IO41")
					(number "31")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IO40")
					(number "32")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IO39")
					(number "33")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IO38")
					(number "34")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "IO37")
					(number "35")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "IO36")
					(number "36")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IO35")
					(number "37")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IO34")
					(number "38")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IO33")
					(number "39")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IO32")
					(number "40")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "IO31")
					(number "41")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "IO30")
					(number "42")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "IO29")
					(number "43")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "IO28")
					(number "44")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "IO27")
					(number "45")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "IO26")
					(number "46")
				)
				(pin input line
					(at 17.78 5.08 180)
					(length 2.54)
					(name "SCL")
					(number "47")
				)
				(pin input line
					(at 17.78 2.54 180)
					(length 2.54)
					(name "SDA")
					(number "48")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "IO42")
					(number "49")
				)
				(pin input line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "GND")
					(number "50")
				)
				(pin input line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "IO13")
					(number "51")
				)
				(pin input line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "IO12")
					(number "52")
				)
				(pin input line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "IO11")
					(number "53")
				)
				(pin input line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "IO10")
					(number "54")
				)
				(pin input line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "IO09")
					(number "55")
				)
				(pin input line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "IO08")
					(number "56")
				)
				(pin input line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "IO07")
					(number "57")
				)
				(pin input line
					(at 17.78 -25.4 180)
					(length 2.54)
					(name "IO06")
					(number "58")
				)
				(pin input line
					(at 17.78 -27.94 180)
					(length 2.54)
					(name "IO05")
					(number "59")
				)
				(pin input line
					(at 17.78 -30.48 180)
					(length 2.54)
					(name "IO04")
					(number "60")
				)
				(pin input line
					(at 17.78 -33.02 180)
					(length 2.54)
					(name "IO03")
					(number "61")
				)
				(pin input line
					(at 17.78 -35.56 180)
					(length 2.54)
					(name "IO02")
					(number "62")
				)
				(pin input line
					(at 17.78 -38.1 180)
					(length 2.54)
					(name "IO01")
					(number "63")
				)
				(pin input line
					(at 17.78 -40.64 180)
					(length 2.54)
					(name "IO00")
					(number "64")
				)
			)
			(symbol "arty_chipKIT_connector_3_0")
			(symbol "arty_chipKIT_connector_3_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "SS")
					(number "25")
				)
				(pin input line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "26")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCK")
					(number "27")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "MISO")
					(number "28")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "MOSI")
					(number "29")
				)
				(pin input line
					(at 16.51 0 180)
					(length 2.54)
					(name "NC")
					(number "30")
				)
			)
			(embedded_fonts no)
		)
)
