(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ASP-134486-01"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 45.72 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ASP-134486-01"
				(at 45.72 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ASP-134486-01"
				(at 45.72 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://suddendocs.samtec.com/prints/asp-134486-01-mkt.pdf?_gl=1*a2d3qa*_ga*MzYxMTM5My4xNjYzOTI3MDkz*_ga_3KFNZC07WW*MTY2NDIwMTUxMC4zLjAuMTY2NDIwMTUxMC42MC4wLjA."
				(at 45.72 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Mezzanine Connector, Vita 57 XMC, Array, Female, 1.27 mm, 10 Rows, 400 Contacts, Surface Mount"
				(at 45.72 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Samtec"
				(at 45.72 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ASP-134486-01"
				(at 45.72 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ASP-134486-01_1_1"
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J1")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "CLK3_{BIDIR}+")
					(number "J2")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "CLK3_{BIDIR}-")
					(number "J3")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "HA03+")
					(number "J6")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "HA03-")
					(number "J7")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J8")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "HA07+")
					(number "J9")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "HA07-")
					(number "J10")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J11")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "HA11+")
					(number "J12")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "HA11-")
					(number "J13")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J14")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "HA14+")
					(number "J15")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "HA14-")
					(number "J16")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J17")
				)
				(pin passive line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "HA18+")
					(number "J18")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "HA18-")
					(number "J19")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J20")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "HA22+")
					(number "J21")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "HA22-")
					(number "J22")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J23")
				)
				(pin passive line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "HB01+")
					(number "J24")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "HB01-")
					(number "J25")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J26")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "HB07+")
					(number "J27")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "HB07-")
					(number "J28")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J29")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "HB11+")
					(number "J30")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "HB11-")
					(number "J31")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J32")
				)
				(pin passive line
					(at 30.48 -69.85 180)
					(length 3.81)
					(name "HB15+")
					(number "J33")
				)
				(pin passive line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "HB15-")
					(number "J34")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J35")
				)
				(pin passive line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "HB18+")
					(number "J36")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "HB18-")
					(number "J37")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J38")
				)
				(pin passive line
					(at 30.48 -85.09 180)
					(length 3.81)
					(name "VIO_{B_M2C}")
					(number "J39")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "J40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VREF_{B_M2C}")
					(number "K1")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K2")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "CLK2_{BIDIR}+")
					(number "K4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CLK2_{BIDIR}-")
					(number "K5")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "HA02+")
					(number "K7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "HA02-")
					(number "K8")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K9")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "HA06+")
					(number "K10")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "HA06-")
					(number "K11")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "HA10+")
					(number "K13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "HA10-")
					(number "K14")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K15")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "HA17_{CC}+")
					(number "K16")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "HA17_{CC}-")
					(number "K17")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K18")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "HA21+")
					(number "K19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "HA21-")
					(number "K20")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K21")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "HA23+")
					(number "K22")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "HA23-")
					(number "K23")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K24")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "HB00_{CC}+")
					(number "K25")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "HB00_{CC}-")
					(number "K26")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K27")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "HB06_{CC}+")
					(number "K28")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "HB06_{CC}-")
					(number "K29")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K30")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "HB10+")
					(number "K31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "HB10-")
					(number "K32")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K33")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "HB14+")
					(number "K34")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "HB14-")
					(number "K35")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K36")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "HB17_{CC}+")
					(number "K37")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "HB17_{CC}-")
					(number "K38")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "K39")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "VIO_{B_M2C}")
					(number "K40")
				)
			)
			(symbol "ASP-134486-01_2_1"
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "CLK1_{M2C}+")
					(number "G2")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "CLK1_{M2C}-")
					(number "G3")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "LA00_{CC}+")
					(number "G6")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "LA00_{CC}-")
					(number "G7")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "LA03+")
					(number "G9")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "LA03-")
					(number "G10")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "LA08+")
					(number "G12")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "LA08-")
					(number "G13")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "LA12+")
					(number "G15")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "LA12-")
					(number "G16")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G17")
				)
				(pin passive line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "LA16+")
					(number "G18")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "LA16-")
					(number "G19")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G20")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "LA20+")
					(number "G21")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "LA20-")
					(number "G22")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G23")
				)
				(pin passive line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "LA22+")
					(number "G24")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "LA22-")
					(number "G25")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G26")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "LA25+")
					(number "G27")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "LA25-")
					(number "G28")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G29")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "LA29+")
					(number "G30")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "LA29-")
					(number "G31")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G32")
				)
				(pin passive line
					(at 30.48 -69.85 180)
					(length 3.81)
					(name "LA31+")
					(number "G33")
				)
				(pin passive line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "LA31-")
					(number "G34")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G35")
				)
				(pin passive line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "LA33+")
					(number "G36")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "LA33-")
					(number "G37")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G38")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "VADJ")
					(number "G39")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "G40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VREF_{A_M2C}")
					(number "H1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{PRSNT_{M2C}}")
					(number "H2")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "CLK0_{M2C}+")
					(number "H4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CLK0_{M2C}-")
					(number "H5")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "LA02+")
					(number "H7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "LA02-")
					(number "H8")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "LA04+")
					(number "H10")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "LA04-")
					(number "H11")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "LA07+")
					(number "H13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "LA07-")
					(number "H14")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H15")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "LA11+")
					(number "H16")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "LA11-")
					(number "H17")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H18")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "LA15+")
					(number "H19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "LA15-")
					(number "H20")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H21")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "LA19+")
					(number "H22")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "LA19-")
					(number "H23")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H24")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LA21+")
					(number "H25")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "LA21-")
					(number "H26")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H27")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "LA24+")
					(number "H28")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "LA24-")
					(number "H29")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H30")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "LA28+")
					(number "H31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "LA28-")
					(number "H32")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H33")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "LA30+")
					(number "H34")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "LA30-")
					(number "H35")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H36")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "LA32+")
					(number "H37")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "LA32-")
					(number "H38")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "H39")
				)
				(pin passive line
					(at 30.48 -85.09 180)
					(length 3.81)
					(name "VADJ")
					(number "H40")
				)
			)
			(symbol "ASP-134486-01_3_1"
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E1")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "HA01_{CC}+")
					(number "E2")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "HA01_{CC}-")
					(number "E3")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "HA05+")
					(number "E6")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "HA05-")
					(number "E7")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "HA09+")
					(number "E9")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "HA09-")
					(number "E10")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "HA13+")
					(number "E12")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "HA13-")
					(number "E13")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E14")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "HA16+")
					(number "E15")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "HA16-")
					(number "E16")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E17")
				)
				(pin passive line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "HA20+")
					(number "E18")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "HA20-")
					(number "E19")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E20")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "HB03+")
					(number "E21")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "HB03-")
					(number "E22")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E23")
				)
				(pin passive line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "HB05+")
					(number "E24")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "HB05-")
					(number "E25")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E26")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "HB09+")
					(number "E27")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "HB09-")
					(number "E28")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E29")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "HB13+")
					(number "E30")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "HB13-")
					(number "E31")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E32")
				)
				(pin passive line
					(at 30.48 -69.85 180)
					(length 3.81)
					(name "HB19+")
					(number "E33")
				)
				(pin passive line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "HB19-")
					(number "E34")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E35")
				)
				(pin passive line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "HB21+")
					(number "E36")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "HB21-")
					(number "E37")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E38")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "VADJ")
					(number "E39")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "E40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "PG_{M2C}")
					(number "F1")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F2")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "HA00_{CC}+")
					(number "F4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "HA00_{CC}-")
					(number "F5")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "HA04+")
					(number "F7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "HA04-")
					(number "F8")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "HA08+")
					(number "F10")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "HA08-")
					(number "F11")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "HA12+")
					(number "F13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "HA12-")
					(number "F14")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F15")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "HA15+")
					(number "F16")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "HA15-")
					(number "F17")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F18")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "HA19+")
					(number "F19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "HA19-")
					(number "F20")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F21")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "HB02+")
					(number "F22")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "HB02-")
					(number "F23")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F24")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "HB04+")
					(number "F25")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "HB04-")
					(number "F26")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F27")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "HB08+")
					(number "F28")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "HB08-")
					(number "F29")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F30")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "HB12+")
					(number "F31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "HB12-")
					(number "F32")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F33")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "HB16+")
					(number "F34")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "HB16-")
					(number "F35")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F36")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "HB20+")
					(number "F37")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "HB20-")
					(number "F38")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "F39")
				)
				(pin passive line
					(at 30.48 -85.09 180)
					(length 3.81)
					(name "VADJ")
					(number "F40")
				)
			)
			(symbol "ASP-134486-01_4_1"
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C1")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "DP0_{C2M}+")
					(number "C2")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "DP0_{C2M}-")
					(number "C3")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "DP0_{M2C}+")
					(number "C6")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "DP0_{M2C}-")
					(number "C7")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C8")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C9")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "LA06+")
					(number "C10")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "LA06-")
					(number "C11")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C12")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C13")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "LA10+")
					(number "C14")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "LA10-")
					(number "C15")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C16")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C17")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "LA14+")
					(number "C18")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "LA14-")
					(number "C19")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C20")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C21")
				)
				(pin passive line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "LA18_{CC}+")
					(number "C22")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "LA18_{CC}-")
					(number "C23")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C24")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C25")
				)
				(pin passive line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "LA27+")
					(number "C26")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "LA27-")
					(number "C27")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C28")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C29")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "SCL")
					(number "C30")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "SDA")
					(number "C31")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C32")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C33")
				)
				(pin passive line
					(at 30.48 -74.93 180)
					(length 3.81)
					(name "GA0")
					(number "C34")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "12P0V")
					(number "C35")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C36")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "12P0V")
					(number "C37")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C38")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "3P3V")
					(number "C39")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "C40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "PG_{C2M}")
					(number "D1")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D2")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "GBTCLK0_{M2C}+")
					(number "D4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "GBTCLK0_{M2C}-")
					(number "D5")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D6")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "LA01_{CC}+")
					(number "D8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "LA01_{CC}-")
					(number "D9")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D10")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "LA05+")
					(number "D11")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "LA05-")
					(number "D12")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "LA09+")
					(number "D14")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "LA09-")
					(number "D15")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D16")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "LA13+")
					(number "D17")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "LA13-")
					(number "D18")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D19")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "LA17_{CC}+")
					(number "D20")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "LA17_{CC}-")
					(number "D21")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D22")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "LA23+")
					(number "D23")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "LA23-")
					(number "D24")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D25")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LA26+")
					(number "D26")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "LA26-")
					(number "D27")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D28")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "TCK")
					(number "D29")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "TDI")
					(number "D30")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "TDO")
					(number "D31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "3P3VAUX")
					(number "D32")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "TMS")
					(number "D33")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "TRST_L")
					(number "D34")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(name "GA1")
					(number "D35")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "3P3V")
					(number "D36")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D37")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "3P3V")
					(number "D38")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "D39")
				)
				(pin passive line
					(at 30.48 -82.55 180)
					(length 3.81)
					(name "3P3V")
					(number "D40")
				)
			)
			(symbol "ASP-134486-01_5_1"
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "DP1_{M2C}+")
					(number "A2")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "DP1_{M2C}-")
					(number "A3")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "DP2_{M2C}+")
					(number "A6")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "DP2_{M2C}-")
					(number "A7")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A8")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A9")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "DP3_{M2C}+")
					(number "A10")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "DP3_{M2C}-")
					(number "A11")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A13")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "DP4_{M2C}+")
					(number "A14")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "DP4_{M2C}-")
					(number "A15")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A16")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A17")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "DP5_{M2C}+")
					(number "A18")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "DP5_{M2C}-")
					(number "A19")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A20")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A21")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "DP1_{C2M}+")
					(number "A22")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "DP1_{C2M}-")
					(number "A23")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A24")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A25")
				)
				(pin passive line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "DP2_{C2M}+")
					(number "A26")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "DP2_{C2M}-")
					(number "A27")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A28")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A29")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "DP3_{C2M}+")
					(number "A30")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "DP3_{C2M}-")
					(number "A31")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A33")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "DP4_{C2M}+")
					(number "A34")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "DP4_{C2M}-")
					(number "A35")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A36")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A37")
				)
				(pin passive line
					(at 30.48 -69.85 180)
					(length 3.81)
					(name "DP5_{C2M}+")
					(number "A38")
				)
				(pin passive line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "DP5_{C2M}-")
					(number "A39")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "A40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "CLK_{DIR}")
					(number "B1")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "DP9_{M2C}+")
					(number "B4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "DP9_{M2C}-")
					(number "B5")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B6")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DP8_{M2C}+")
					(number "B8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DP8_{M2C}-")
					(number "B9")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B10")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "DP7_{M2C}+")
					(number "B12")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "DP7_{M2C}-")
					(number "B13")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B14")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B15")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DP6_{M2C}+")
					(number "B16")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DP6_{M2C}-")
					(number "B17")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B18")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B19")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "GBTCLK1_{M2C}+")
					(number "B20")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "GBTCLK1_{M2C}-")
					(number "B21")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B23")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "DP9_{C2M}+")
					(number "B24")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "DP9_{C2M}-")
					(number "B25")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B26")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B27")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DP8_{C2M}+")
					(number "B28")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DP8_{C2M}-")
					(number "B29")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B30")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B31")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "DP7_{C2M}+")
					(number "B32")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "DP7_{C2M}-")
					(number "B33")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B34")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B35")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "DP6_{C2M}+")
					(number "B36")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DP6_{C2M}-")
					(number "B37")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B38")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 3.81)
					(name "GND")
					(number "B39")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "RES0")
					(number "B40")
				)
			)
			(embedded_fonts no)
		)
)
