(footprint "Conn_FMC_Samtec_ASP_134602-01"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -29.45 9.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_FMC_Samtec_ASP_134602-01"
		(at -29.3 10.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -29.33 11.95 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -29.33 13.15 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -29.33 14.35 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -26.705 3.09)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.675 0.04)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd circle
		(at 25.25 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A2" smd circle
		(at 23.98 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A3" smd circle
		(at 22.71 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A4" smd circle
		(at 21.44 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A5" smd circle
		(at 20.17 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A6" smd circle
		(at 18.9 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A7" smd circle
		(at 17.63 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A8" smd circle
		(at 16.36 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A9" smd circle
		(at 15.09 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A10" smd circle
		(at 13.82 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A11" smd circle
		(at 12.55 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A12" smd circle
		(at 11.28 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A13" smd circle
		(at 10.01 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A14" smd circle
		(at 8.74 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A15" smd circle
		(at 7.47 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A16" smd circle
		(at 6.2 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A17" smd circle
		(at 4.93 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A18" smd circle
		(at 3.66 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A19" smd circle
		(at 2.39 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A20" smd circle
		(at 1.12 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A21" smd circle
		(at -0.15 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A22" smd circle
		(at -1.42 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A23" smd circle
		(at -2.69 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A24" smd circle
		(at -3.96 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A25" smd circle
		(at -5.23 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A26" smd circle
		(at -6.5 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A27" smd circle
		(at -7.77 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A28" smd circle
		(at -9.04 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A29" smd circle
		(at -10.31 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A30" smd circle
		(at -11.58 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A31" smd circle
		(at -12.85 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A32" smd circle
		(at -14.12 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A33" smd circle
		(at -15.39 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A34" smd circle
		(at -16.66 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A35" smd circle
		(at -17.93 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A36" smd circle
		(at -19.2 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A37" smd circle
		(at -20.47 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A38" smd circle
		(at -21.74 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A39" smd circle
		(at -23.01 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "A40" smd circle
		(at -24.28 -5.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B1" smd circle
		(at 25.25 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B2" smd circle
		(at 23.98 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B3" smd circle
		(at 22.71 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B4" smd circle
		(at 21.44 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B5" smd circle
		(at 20.17 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B6" smd circle
		(at 18.9 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B7" smd circle
		(at 17.63 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B8" smd circle
		(at 16.36 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B9" smd circle
		(at 15.09 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B10" smd circle
		(at 13.82 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B11" smd circle
		(at 12.55 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B12" smd circle
		(at 11.28 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B13" smd circle
		(at 10.01 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B14" smd circle
		(at 8.74 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B15" smd circle
		(at 7.47 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B16" smd circle
		(at 6.2 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B17" smd circle
		(at 4.93 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B18" smd circle
		(at 3.66 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B19" smd circle
		(at 2.39 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B20" smd circle
		(at 1.12 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B21" smd circle
		(at -0.15 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B22" smd circle
		(at -1.42 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B23" smd circle
		(at -2.69 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B24" smd circle
		(at -3.96 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B25" smd circle
		(at -5.23 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B26" smd circle
		(at -6.5 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B27" smd circle
		(at -7.77 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B28" smd circle
		(at -9.04 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B29" smd circle
		(at -10.31 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B30" smd circle
		(at -11.58 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B31" smd circle
		(at -12.85 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B32" smd circle
		(at -14.12 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B33" smd circle
		(at -15.39 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B34" smd circle
		(at -16.66 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B35" smd circle
		(at -17.93 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B36" smd circle
		(at -19.2 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B37" smd circle
		(at -20.47 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B38" smd circle
		(at -21.74 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B39" smd circle
		(at -23.01 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "B40" smd circle
		(at -24.28 -4.405)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C1" smd circle
		(at 25.25 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C2" smd circle
		(at 23.98 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C3" smd circle
		(at 22.71 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C4" smd circle
		(at 21.44 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C5" smd circle
		(at 20.17 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C6" smd circle
		(at 18.9 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C7" smd circle
		(at 17.63 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C8" smd circle
		(at 16.36 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C9" smd circle
		(at 15.09 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C10" smd circle
		(at 13.82 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C11" smd circle
		(at 12.55 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C12" smd circle
		(at 11.28 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C13" smd circle
		(at 10.01 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C14" smd circle
		(at 8.74 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C15" smd circle
		(at 7.47 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C16" smd circle
		(at 6.2 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C17" smd circle
		(at 4.93 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C18" smd circle
		(at 3.66 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C19" smd circle
		(at 2.39 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C20" smd circle
		(at 1.12 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C21" smd circle
		(at -0.15 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C22" smd circle
		(at -1.42 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C23" smd circle
		(at -2.69 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C24" smd circle
		(at -3.96 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C25" smd circle
		(at -5.23 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C26" smd circle
		(at -6.5 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C27" smd circle
		(at -7.77 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C28" smd circle
		(at -9.04 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C29" smd circle
		(at -10.31 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C30" smd circle
		(at -11.58 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C31" smd circle
		(at -12.85 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C32" smd circle
		(at -14.12 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C33" smd circle
		(at -15.39 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C34" smd circle
		(at -16.66 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C35" smd circle
		(at -17.93 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C36" smd circle
		(at -19.2 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C37" smd circle
		(at -20.47 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C38" smd circle
		(at -21.74 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C39" smd circle
		(at -23.01 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "C40" smd circle
		(at -24.28 -3.135)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D1" smd circle
		(at 25.25 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D2" smd circle
		(at 23.98 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D3" smd circle
		(at 22.71 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D4" smd circle
		(at 21.44 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D5" smd circle
		(at 20.17 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D6" smd circle
		(at 18.9 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D7" smd circle
		(at 17.63 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D8" smd circle
		(at 16.36 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D9" smd circle
		(at 15.09 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D10" smd circle
		(at 13.82 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D11" smd circle
		(at 12.55 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D12" smd circle
		(at 11.28 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D13" smd circle
		(at 10.01 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D14" smd circle
		(at 8.74 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D15" smd circle
		(at 7.47 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D16" smd circle
		(at 6.2 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D17" smd circle
		(at 4.93 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D18" smd circle
		(at 3.66 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D19" smd circle
		(at 2.39 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D20" smd circle
		(at 1.12 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D21" smd circle
		(at -0.15 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D22" smd circle
		(at -1.42 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D23" smd circle
		(at -2.69 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D24" smd circle
		(at -3.96 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D25" smd circle
		(at -5.23 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D26" smd circle
		(at -6.5 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D27" smd circle
		(at -7.77 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D28" smd circle
		(at -9.04 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D29" smd circle
		(at -10.31 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D30" smd circle
		(at -11.58 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D31" smd circle
		(at -12.85 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D32" smd circle
		(at -14.12 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D33" smd circle
		(at -15.39 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D34" smd circle
		(at -16.66 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D35" smd circle
		(at -17.93 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D36" smd circle
		(at -19.2 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D37" smd circle
		(at -20.47 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D38" smd circle
		(at -21.74 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D39" smd circle
		(at -23.01 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "D40" smd circle
		(at -24.28 -1.865)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E1" smd circle
		(at 25.25 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E2" smd circle
		(at 23.98 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E3" smd circle
		(at 22.71 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E4" smd circle
		(at 21.44 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E5" smd circle
		(at 20.17 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E6" smd circle
		(at 18.9 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E7" smd circle
		(at 17.63 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E8" smd circle
		(at 16.36 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E9" smd circle
		(at 15.09 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E10" smd circle
		(at 13.82 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E11" smd circle
		(at 12.55 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E12" smd circle
		(at 11.28 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E13" smd circle
		(at 10.01 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E14" smd circle
		(at 8.74 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E15" smd circle
		(at 7.47 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E16" smd circle
		(at 6.2 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E17" smd circle
		(at 4.93 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E18" smd circle
		(at 3.66 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E19" smd circle
		(at 2.39 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E20" smd circle
		(at 1.12 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E21" smd circle
		(at -0.15 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E22" smd circle
		(at -1.42 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E23" smd circle
		(at -2.69 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E24" smd circle
		(at -3.96 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E25" smd circle
		(at -5.23 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E26" smd circle
		(at -6.5 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E27" smd circle
		(at -7.77 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E28" smd circle
		(at -9.04 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E29" smd circle
		(at -10.31 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E30" smd circle
		(at -11.58 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E31" smd circle
		(at -12.85 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E32" smd circle
		(at -14.12 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E33" smd circle
		(at -15.39 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E34" smd circle
		(at -16.66 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E35" smd circle
		(at -17.93 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E36" smd circle
		(at -19.2 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E37" smd circle
		(at -20.47 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E38" smd circle
		(at -21.74 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E39" smd circle
		(at -23.01 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "E40" smd circle
		(at -24.28 -0.595)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F1" smd circle
		(at 25.25 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F2" smd circle
		(at 23.98 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F3" smd circle
		(at 22.71 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F4" smd circle
		(at 21.44 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F5" smd circle
		(at 20.17 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F6" smd circle
		(at 18.9 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F7" smd circle
		(at 17.63 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F8" smd circle
		(at 16.36 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F9" smd circle
		(at 15.09 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F10" smd circle
		(at 13.82 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F11" smd circle
		(at 12.55 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F12" smd circle
		(at 11.28 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F13" smd circle
		(at 10.01 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F14" smd circle
		(at 8.74 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F15" smd circle
		(at 7.47 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F16" smd circle
		(at 6.2 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F17" smd circle
		(at 4.93 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F18" smd circle
		(at 3.66 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F19" smd circle
		(at 2.39 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F20" smd circle
		(at 1.12 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F21" smd circle
		(at -0.15 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F22" smd circle
		(at -1.42 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F23" smd circle
		(at -2.69 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F24" smd circle
		(at -3.96 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F25" smd circle
		(at -5.23 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F26" smd circle
		(at -6.5 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F27" smd circle
		(at -7.77 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F28" smd circle
		(at -9.04 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F29" smd circle
		(at -10.31 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F30" smd circle
		(at -11.58 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F31" smd circle
		(at -12.85 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F32" smd circle
		(at -14.12 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F33" smd circle
		(at -15.39 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F34" smd circle
		(at -16.66 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F35" smd circle
		(at -17.93 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F36" smd circle
		(at -19.2 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F37" smd circle
		(at -20.47 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F38" smd circle
		(at -21.74 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F39" smd circle
		(at -23.01 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "F40" smd circle
		(at -24.28 0.675)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G1" smd circle
		(at 25.25 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G2" smd circle
		(at 23.98 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G3" smd circle
		(at 22.71 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G4" smd circle
		(at 21.44 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G5" smd circle
		(at 20.17 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G6" smd circle
		(at 18.9 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G7" smd circle
		(at 17.63 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G8" smd circle
		(at 16.36 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G9" smd circle
		(at 15.09 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G10" smd circle
		(at 13.82 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G11" smd circle
		(at 12.55 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G12" smd circle
		(at 11.28 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G13" smd circle
		(at 10.01 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G14" smd circle
		(at 8.74 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G15" smd circle
		(at 7.47 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G16" smd circle
		(at 6.2 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G17" smd circle
		(at 4.93 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G18" smd circle
		(at 3.66 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G19" smd circle
		(at 2.39 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G20" smd circle
		(at 1.12 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G21" smd circle
		(at -0.15 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G22" smd circle
		(at -1.42 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G23" smd circle
		(at -2.69 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G24" smd circle
		(at -3.96 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G25" smd circle
		(at -5.23 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G26" smd circle
		(at -6.5 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G27" smd circle
		(at -7.77 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G28" smd circle
		(at -9.04 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G29" smd circle
		(at -10.31 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G30" smd circle
		(at -11.58 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G31" smd circle
		(at -12.85 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G32" smd circle
		(at -14.12 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G33" smd circle
		(at -15.39 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G34" smd circle
		(at -16.66 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G35" smd circle
		(at -17.93 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G36" smd circle
		(at -19.2 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G37" smd circle
		(at -20.47 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G38" smd circle
		(at -21.74 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G39" smd circle
		(at -23.01 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "G40" smd circle
		(at -24.28 1.945)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H1" smd circle
		(at 25.25 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H2" smd circle
		(at 23.98 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H3" smd circle
		(at 22.71 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H4" smd circle
		(at 21.44 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H5" smd circle
		(at 20.17 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H6" smd circle
		(at 18.9 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H7" smd circle
		(at 17.63 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H8" smd circle
		(at 16.36 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H9" smd circle
		(at 15.09 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H10" smd circle
		(at 13.82 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H11" smd circle
		(at 12.55 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H12" smd circle
		(at 11.28 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H13" smd circle
		(at 10.01 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H14" smd circle
		(at 8.74 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H15" smd circle
		(at 7.47 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H16" smd circle
		(at 6.2 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H17" smd circle
		(at 4.93 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H18" smd circle
		(at 3.66 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H19" smd circle
		(at 2.39 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H20" smd circle
		(at 1.12 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H21" smd circle
		(at -0.15 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H22" smd circle
		(at -1.42 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H23" smd circle
		(at -2.69 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H24" smd circle
		(at -3.96 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H25" smd circle
		(at -5.23 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H26" smd circle
		(at -6.5 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H27" smd circle
		(at -7.77 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H28" smd circle
		(at -9.04 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H29" smd circle
		(at -10.31 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H30" smd circle
		(at -11.58 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H31" smd circle
		(at -12.85 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H32" smd circle
		(at -14.12 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H33" smd circle
		(at -15.39 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H34" smd circle
		(at -16.66 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H35" smd circle
		(at -17.93 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H36" smd circle
		(at -19.2 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H37" smd circle
		(at -20.47 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H38" smd circle
		(at -21.74 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H39" smd circle
		(at -23.01 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "H40" smd circle
		(at -24.28 3.215)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J1" smd circle
		(at 25.25 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J2" smd circle
		(at 23.98 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J3" smd circle
		(at 22.71 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J4" smd circle
		(at 21.44 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J5" smd circle
		(at 20.17 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J6" smd circle
		(at 18.9 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J7" smd circle
		(at 17.63 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J8" smd circle
		(at 16.36 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J9" smd circle
		(at 15.09 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J10" smd circle
		(at 13.82 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J11" smd circle
		(at 12.55 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J12" smd circle
		(at 11.28 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J13" smd circle
		(at 10.01 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J14" smd circle
		(at 8.74 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J15" smd circle
		(at 7.47 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J16" smd circle
		(at 6.2 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J17" smd circle
		(at 4.93 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J18" smd circle
		(at 3.66 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J19" smd circle
		(at 2.39 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J20" smd circle
		(at 1.12 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J21" smd circle
		(at -0.15 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J22" smd circle
		(at -1.42 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J23" smd circle
		(at -2.69 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J24" smd circle
		(at -3.96 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J25" smd circle
		(at -5.23 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J26" smd circle
		(at -6.5 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J27" smd circle
		(at -7.77 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J28" smd circle
		(at -9.04 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J29" smd circle
		(at -10.31 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J30" smd circle
		(at -11.58 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J31" smd circle
		(at -12.85 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J32" smd circle
		(at -14.12 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J33" smd circle
		(at -15.39 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J34" smd circle
		(at -16.66 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J35" smd circle
		(at -17.93 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J36" smd circle
		(at -19.2 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J37" smd circle
		(at -20.47 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J38" smd circle
		(at -21.74 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J39" smd circle
		(at -23.01 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "J40" smd circle
		(at -24.28 4.485)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K1" smd circle
		(at 25.25 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K2" smd circle
		(at 23.98 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K3" smd circle
		(at 22.71 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K4" smd circle
		(at 21.44 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K5" smd circle
		(at 20.17 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K6" smd circle
		(at 18.9 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K7" smd circle
		(at 17.63 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K8" smd circle
		(at 16.36 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K9" smd circle
		(at 15.09 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K10" smd circle
		(at 13.82 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K11" smd circle
		(at 12.55 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K12" smd circle
		(at 11.28 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K13" smd circle
		(at 10.01 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K14" smd circle
		(at 8.74 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K15" smd circle
		(at 7.47 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K16" smd circle
		(at 6.2 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K17" smd circle
		(at 4.93 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K18" smd circle
		(at 3.66 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K19" smd circle
		(at 2.39 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K20" smd circle
		(at 1.12 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K21" smd circle
		(at -0.15 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K22" smd circle
		(at -1.42 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K23" smd circle
		(at -2.69 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K24" smd circle
		(at -3.96 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K25" smd circle
		(at -5.23 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K26" smd circle
		(at -6.5 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K27" smd circle
		(at -7.77 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K28" smd circle
		(at -9.04 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K29" smd circle
		(at -10.31 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K30" smd circle
		(at -11.58 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K31" smd circle
		(at -12.85 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K32" smd circle
		(at -14.12 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K33" smd circle
		(at -15.39 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K34" smd circle
		(at -16.66 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K35" smd circle
		(at -17.93 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K36" smd circle
		(at -19.2 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K37" smd circle
		(at -20.47 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K38" smd circle
		(at -21.74 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K39" smd circle
		(at -23.01 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "K40" smd circle
		(at -24.28 5.755)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
	(model "antmicro_asp_134602_01.glb"
		(offset
			(xyz 0.444 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 180 180)
		)
	)
)
