(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 36.83 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_Samtec_ASP_10x40_ASP-134602-01"
				(at 36.83 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_Samtec_ASP_10x40_ASP-134602-01"
				(at 36.83 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://suddendocs.samtec.com/prints/asp-134602-01-mkt.pdf"
				(at 36.83 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Mezzanine Connector, Array, 1.27 mm, 10 Rows, 400 Contacts, Surface Mount"
				(at 36.83 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ASP-134602-01"
				(at 36.83 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Samtec"
				(at 36.83 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "A1")
					(number "A1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "A2")
					(number "A2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "A3")
					(number "A3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "A4")
					(number "A4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "A5")
					(number "A5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "A6")
					(number "A6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "A7")
					(number "A7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "A8")
					(number "A8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "A9")
					(number "A9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "A10")
					(number "A10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "A11")
					(number "A11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "A12")
					(number "A12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "A13")
					(number "A13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "A14")
					(number "A14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "A15")
					(number "A15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "A16")
					(number "A16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "A17")
					(number "A17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "A18")
					(number "A18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "A19")
					(number "A19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "A20")
					(number "A20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "A21")
					(number "A21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "A22")
					(number "A22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "A23")
					(number "A23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "A24")
					(number "A24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "A25")
					(number "A25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "A26")
					(number "A26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "A27")
					(number "A27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "A28")
					(number "A28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "A29")
					(number "A29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "A30")
					(number "A30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "A31")
					(number "A31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "A32")
					(number "A32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "A33")
					(number "A33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "A34")
					(number "A34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "A35")
					(number "A35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "A36")
					(number "A36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "A37")
					(number "A37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "A38")
					(number "A38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "A39")
					(number "A39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "A40")
					(number "A40")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "B1")
					(number "B1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "B2")
					(number "B2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "B3")
					(number "B3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "B4")
					(number "B4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "B5")
					(number "B5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "B6")
					(number "B6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "B7")
					(number "B7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "B8")
					(number "B8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "B9")
					(number "B9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "B10")
					(number "B10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "B11")
					(number "B11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "B12")
					(number "B12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "B13")
					(number "B13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "B14")
					(number "B14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "B15")
					(number "B15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "B16")
					(number "B16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "B17")
					(number "B17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "B18")
					(number "B18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "B19")
					(number "B19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "B20")
					(number "B20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "B21")
					(number "B21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "B22")
					(number "B22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "B23")
					(number "B23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "B24")
					(number "B24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "B25")
					(number "B25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "B26")
					(number "B26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "B27")
					(number "B27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "B28")
					(number "B28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "B29")
					(number "B29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "B30")
					(number "B30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "B31")
					(number "B31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "B32")
					(number "B32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "B33")
					(number "B33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "B34")
					(number "B34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "B35")
					(number "B35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "B36")
					(number "B36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "B37")
					(number "B37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "B38")
					(number "B38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "B39")
					(number "B39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "B40")
					(number "B40")
				)
			)
			(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01_2_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "C1")
					(number "C1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "C2")
					(number "C2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "C3")
					(number "C3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "C4")
					(number "C4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "C5")
					(number "C5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "C6")
					(number "C6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "C7")
					(number "C7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "C8")
					(number "C8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "C9")
					(number "C9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "C10")
					(number "C10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "C11")
					(number "C11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "C12")
					(number "C12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "C13")
					(number "C13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "C14")
					(number "C14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "C15")
					(number "C15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "C16")
					(number "C16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "C17")
					(number "C17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "C18")
					(number "C18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "C19")
					(number "C19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "C20")
					(number "C20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "C21")
					(number "C21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "C22")
					(number "C22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "C23")
					(number "C23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "C24")
					(number "C24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "C25")
					(number "C25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "C26")
					(number "C26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "C27")
					(number "C27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "C28")
					(number "C28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "C29")
					(number "C29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "C30")
					(number "C30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "C31")
					(number "C31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "C32")
					(number "C32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "C33")
					(number "C33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "C34")
					(number "C34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "C35")
					(number "C35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "C36")
					(number "C36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "C37")
					(number "C37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "C38")
					(number "C38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "C39")
					(number "C39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "C40")
					(number "C40")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "D1")
					(number "D1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "D2")
					(number "D2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "D3")
					(number "D3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "D4")
					(number "D4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "D5")
					(number "D5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "D6")
					(number "D6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "D7")
					(number "D7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "D8")
					(number "D8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "D9")
					(number "D9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "D10")
					(number "D10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "D11")
					(number "D11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "D12")
					(number "D12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "D13")
					(number "D13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "D14")
					(number "D14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "D15")
					(number "D15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "D16")
					(number "D16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "D17")
					(number "D17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "D18")
					(number "D18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "D19")
					(number "D19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "D20")
					(number "D20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "D21")
					(number "D21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "D22")
					(number "D22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "D23")
					(number "D23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "D24")
					(number "D24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "D25")
					(number "D25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "D26")
					(number "D26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "D27")
					(number "D27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "D28")
					(number "D28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "D29")
					(number "D29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "D30")
					(number "D30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "D31")
					(number "D31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "D32")
					(number "D32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "D33")
					(number "D33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "D34")
					(number "D34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "D35")
					(number "D35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "D36")
					(number "D36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "D37")
					(number "D37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "D38")
					(number "D38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "D39")
					(number "D39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "D40")
					(number "D40")
				)
			)
			(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01_3_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "E1")
					(number "E1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "E2")
					(number "E2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "E3")
					(number "E3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "E4")
					(number "E4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "E5")
					(number "E5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "E6")
					(number "E6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "E7")
					(number "E7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "E8")
					(number "E8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "E9")
					(number "E9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "E10")
					(number "E10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "E11")
					(number "E11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "E12")
					(number "E12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "E13")
					(number "E13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "E14")
					(number "E14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "E15")
					(number "E15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "E16")
					(number "E16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "E17")
					(number "E17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "E18")
					(number "E18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "E19")
					(number "E19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "E20")
					(number "E20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "E21")
					(number "E21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "E22")
					(number "E22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "E23")
					(number "E23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "E24")
					(number "E24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "E25")
					(number "E25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "E26")
					(number "E26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "E27")
					(number "E27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "E28")
					(number "E28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "E29")
					(number "E29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "E30")
					(number "E30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "E31")
					(number "E31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "E32")
					(number "E32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "E33")
					(number "E33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "E34")
					(number "E34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "E35")
					(number "E35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "E36")
					(number "E36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "E37")
					(number "E37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "E38")
					(number "E38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "E39")
					(number "E39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "E40")
					(number "E40")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "F1")
					(number "F1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "F2")
					(number "F2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "F3")
					(number "F3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "F4")
					(number "F4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "F5")
					(number "F5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "F6")
					(number "F6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "F7")
					(number "F7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "F8")
					(number "F8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "F9")
					(number "F9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "F10")
					(number "F10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "F11")
					(number "F11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "F12")
					(number "F12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "F13")
					(number "F13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "F14")
					(number "F14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "F15")
					(number "F15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "F16")
					(number "F16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "F17")
					(number "F17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "F18")
					(number "F18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "F19")
					(number "F19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "F20")
					(number "F20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "F21")
					(number "F21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "F22")
					(number "F22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "F23")
					(number "F23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "F24")
					(number "F24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "F25")
					(number "F25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "F26")
					(number "F26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "F27")
					(number "F27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "F28")
					(number "F28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "F29")
					(number "F29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "F30")
					(number "F30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "F31")
					(number "F31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "F32")
					(number "F32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "F33")
					(number "F33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "F34")
					(number "F34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "F35")
					(number "F35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "F36")
					(number "F36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "F37")
					(number "F37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "F38")
					(number "F38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "F39")
					(number "F39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "F40")
					(number "F40")
				)
			)
			(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01_4_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "G1")
					(number "G1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "G2")
					(number "G2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "G3")
					(number "G3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "G4")
					(number "G4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "G5")
					(number "G5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "G6")
					(number "G6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "G7")
					(number "G7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "G8")
					(number "G8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "G9")
					(number "G9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "G10")
					(number "G10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "G11")
					(number "G11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "G12")
					(number "G12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "G13")
					(number "G13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "G14")
					(number "G14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "G15")
					(number "G15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "G16")
					(number "G16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "G17")
					(number "G17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "G18")
					(number "G18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "G19")
					(number "G19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "G20")
					(number "G20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "G21")
					(number "G21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "G22")
					(number "G22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "G23")
					(number "G23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "G24")
					(number "G24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "G25")
					(number "G25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "G26")
					(number "G26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "G27")
					(number "G27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "G28")
					(number "G28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "G29")
					(number "G29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "G30")
					(number "G30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "G31")
					(number "G31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "G32")
					(number "G32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "G33")
					(number "G33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "G34")
					(number "G34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "G35")
					(number "G35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "G36")
					(number "G36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "G37")
					(number "G37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "G38")
					(number "G38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "G39")
					(number "G39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "G40")
					(number "G40")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "H1")
					(number "H1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "H2")
					(number "H2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "H3")
					(number "H3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "H4")
					(number "H4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "H5")
					(number "H5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "H6")
					(number "H6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "H7")
					(number "H7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "H8")
					(number "H8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "H9")
					(number "H9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "H10")
					(number "H10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "H11")
					(number "H11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "H12")
					(number "H12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "H13")
					(number "H13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "H14")
					(number "H14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "H15")
					(number "H15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "H16")
					(number "H16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "H17")
					(number "H17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "H18")
					(number "H18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "H19")
					(number "H19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "H20")
					(number "H20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "H21")
					(number "H21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "H22")
					(number "H22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "H23")
					(number "H23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "H24")
					(number "H24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "H25")
					(number "H25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "H26")
					(number "H26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "H27")
					(number "H27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "H28")
					(number "H28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "H29")
					(number "H29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "H30")
					(number "H30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "H31")
					(number "H31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "H32")
					(number "H32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "H33")
					(number "H33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "H34")
					(number "H34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "H35")
					(number "H35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "H36")
					(number "H36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "H37")
					(number "H37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "H38")
					(number "H38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "H39")
					(number "H39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "H40")
					(number "H40")
				)
			)
			(symbol "Socket_Samtec_ASP_10x40_ASP-134602-01_5_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "J1")
					(number "J1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "J2")
					(number "J2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "J3")
					(number "J3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "J4")
					(number "J4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "J5")
					(number "J5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "J6")
					(number "J6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "J7")
					(number "J7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "J8")
					(number "J8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "J9")
					(number "J9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "J10")
					(number "J10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "J11")
					(number "J11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "J12")
					(number "J12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "J13")
					(number "J13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "J14")
					(number "J14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "J15")
					(number "J15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "J16")
					(number "J16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "J17")
					(number "J17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "J18")
					(number "J18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "J19")
					(number "J19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "J20")
					(number "J20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "J21")
					(number "J21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "J22")
					(number "J22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "J23")
					(number "J23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "J24")
					(number "J24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "J25")
					(number "J25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "J26")
					(number "J26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "J27")
					(number "J27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "J28")
					(number "J28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "J29")
					(number "J29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "J30")
					(number "J30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "J31")
					(number "J31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "J32")
					(number "J32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "J33")
					(number "J33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "J34")
					(number "J34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "J35")
					(number "J35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "J36")
					(number "J36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "J37")
					(number "J37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "J38")
					(number "J38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "J39")
					(number "J39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "J40")
					(number "J40")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "K1")
					(number "K1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "K2")
					(number "K2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "K3")
					(number "K3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "K4")
					(number "K4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "K5")
					(number "K5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "K6")
					(number "K6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "K7")
					(number "K7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "K8")
					(number "K8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "K9")
					(number "K9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "K10")
					(number "K10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "K11")
					(number "K11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "K12")
					(number "K12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "K13")
					(number "K13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "K14")
					(number "K14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "K15")
					(number "K15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "K16")
					(number "K16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "K17")
					(number "K17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "K18")
					(number "K18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "K19")
					(number "K19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "K20")
					(number "K20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "K21")
					(number "K21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "K22")
					(number "K22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "K23")
					(number "K23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "K24")
					(number "K24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "K25")
					(number "K25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "K26")
					(number "K26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "K27")
					(number "K27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "K28")
					(number "K28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "K29")
					(number "K29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "K30")
					(number "K30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "K31")
					(number "K31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "K32")
					(number "K32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "K33")
					(number "K33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "K34")
					(number "K34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "K35")
					(number "K35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "K36")
					(number "K36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "K37")
					(number "K37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "K38")
					(number "K38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "K39")
					(number "K39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "K40")
					(number "K40")
				)
			)
			(embedded_fonts no)
		)
)
