(footprint "ASP-134603-01_mounting_holes"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -28.97 -6.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "ASP-134603-01_mounting_holes"
		(at 0 8.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -29.02 8.8 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -29.02 10 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -29.02 11.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -31.495 -2.045)
		(size 6 6)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -27.185 -0.045)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.195 3.005)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 31.505 -2.045)
		(size 6 6)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "C1" smd circle
		(at 24.77 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C2" smd circle
		(at 23.5 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C3" smd circle
		(at 22.23 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C4" smd circle
		(at 20.96 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C5" smd circle
		(at 19.69 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C6" smd circle
		(at 18.42 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C7" smd circle
		(at 17.15 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C8" smd circle
		(at 15.88 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C9" smd circle
		(at 14.61 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C10" smd circle
		(at 13.34 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C11" smd circle
		(at 12.07 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C12" smd circle
		(at 10.8 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C13" smd circle
		(at 9.53 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C14" smd circle
		(at 8.26 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C15" smd circle
		(at 6.99 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C16" smd circle
		(at 5.72 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C17" smd circle
		(at 4.45 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C18" smd circle
		(at 3.18 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C19" smd circle
		(at 1.91 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C20" smd circle
		(at 0.64 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C21" smd circle
		(at -0.63 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C22" smd circle
		(at -1.9 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C23" smd circle
		(at -3.17 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C24" smd circle
		(at -4.44 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C25" smd circle
		(at -5.71 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C26" smd circle
		(at -6.98 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C27" smd circle
		(at -8.25 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C28" smd circle
		(at -9.52 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C29" smd circle
		(at -10.79 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C30" smd circle
		(at -12.06 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C31" smd circle
		(at -13.33 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C32" smd circle
		(at -14.6 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C33" smd circle
		(at -15.87 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C34" smd circle
		(at -17.14 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C35" smd circle
		(at -18.41 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C36" smd circle
		(at -19.68 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C37" smd circle
		(at -20.95 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C38" smd circle
		(at -22.22 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C39" smd circle
		(at -23.49 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "C40" smd circle
		(at -24.76 3.13)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D1" smd circle
		(at 24.77 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D2" smd circle
		(at 23.5 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D3" smd circle
		(at 22.23 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D4" smd circle
		(at 20.96 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D5" smd circle
		(at 19.69 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D6" smd circle
		(at 18.42 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D7" smd circle
		(at 17.15 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D8" smd circle
		(at 15.88 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D9" smd circle
		(at 14.61 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D10" smd circle
		(at 13.34 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D11" smd circle
		(at 12.07 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D12" smd circle
		(at 10.8 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D13" smd circle
		(at 9.53 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D14" smd circle
		(at 8.26 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D15" smd circle
		(at 6.99 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D16" smd circle
		(at 5.72 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D17" smd circle
		(at 4.45 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D18" smd circle
		(at 3.18 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D19" smd circle
		(at 1.91 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D20" smd circle
		(at 0.64 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D21" smd circle
		(at -0.63 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D22" smd circle
		(at -1.9 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D23" smd circle
		(at -3.17 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D24" smd circle
		(at -4.44 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D25" smd circle
		(at -5.71 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D26" smd circle
		(at -6.98 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D27" smd circle
		(at -8.25 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D28" smd circle
		(at -9.52 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D29" smd circle
		(at -10.79 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D30" smd circle
		(at -12.06 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D31" smd circle
		(at -13.33 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D32" smd circle
		(at -14.6 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D33" smd circle
		(at -15.87 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D34" smd circle
		(at -17.14 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D35" smd circle
		(at -18.41 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D36" smd circle
		(at -19.68 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D37" smd circle
		(at -20.95 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D38" smd circle
		(at -22.22 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D39" smd circle
		(at -23.49 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "D40" smd circle
		(at -24.76 1.86)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G1" smd circle
		(at 24.77 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G2" smd circle
		(at 23.5 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G3" smd circle
		(at 22.23 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G4" smd circle
		(at 20.96 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G5" smd circle
		(at 19.69 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G6" smd circle
		(at 18.42 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G7" smd circle
		(at 17.15 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G8" smd circle
		(at 15.88 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G9" smd circle
		(at 14.61 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G10" smd circle
		(at 13.34 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G11" smd circle
		(at 12.07 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G12" smd circle
		(at 10.8 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G13" smd circle
		(at 9.53 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G14" smd circle
		(at 8.26 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G15" smd circle
		(at 6.99 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G16" smd circle
		(at 5.72 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G17" smd circle
		(at 4.45 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G18" smd circle
		(at 3.18 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G19" smd circle
		(at 1.91 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G20" smd circle
		(at 0.64 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G21" smd circle
		(at -0.63 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G22" smd circle
		(at -1.9 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G23" smd circle
		(at -3.17 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G24" smd circle
		(at -4.44 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G25" smd circle
		(at -5.71 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G26" smd circle
		(at -6.98 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G27" smd circle
		(at -8.25 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G28" smd circle
		(at -9.52 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G29" smd circle
		(at -10.79 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G30" smd circle
		(at -12.06 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G31" smd circle
		(at -13.33 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G32" smd circle
		(at -14.6 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G33" smd circle
		(at -15.87 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G34" smd circle
		(at -17.14 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G35" smd circle
		(at -18.41 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G36" smd circle
		(at -19.68 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G37" smd circle
		(at -20.95 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G38" smd circle
		(at -22.22 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G39" smd circle
		(at -23.49 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "G40" smd circle
		(at -24.76 -1.95)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H1" smd circle
		(at 24.77 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H2" smd circle
		(at 23.5 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H3" smd circle
		(at 22.23 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H4" smd circle
		(at 20.96 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H5" smd circle
		(at 19.69 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H6" smd circle
		(at 18.42 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H7" smd circle
		(at 17.15 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H8" smd circle
		(at 15.88 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H9" smd circle
		(at 14.61 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H10" smd circle
		(at 13.34 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H11" smd circle
		(at 12.07 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H12" smd circle
		(at 10.8 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H13" smd circle
		(at 9.53 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H14" smd circle
		(at 8.26 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H15" smd circle
		(at 6.99 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H16" smd circle
		(at 5.72 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H17" smd circle
		(at 4.45 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H18" smd circle
		(at 3.18 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H19" smd circle
		(at 1.91 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H20" smd circle
		(at 0.64 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H21" smd circle
		(at -0.63 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H22" smd circle
		(at -1.9 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H23" smd circle
		(at -3.17 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H24" smd circle
		(at -4.44 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H25" smd circle
		(at -5.71 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H26" smd circle
		(at -6.98 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H27" smd circle
		(at -8.25 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H28" smd circle
		(at -9.52 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H29" smd circle
		(at -10.79 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H30" smd circle
		(at -12.06 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H31" smd circle
		(at -13.33 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H32" smd circle
		(at -14.6 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H33" smd circle
		(at -15.87 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H34" smd circle
		(at -17.14 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H35" smd circle
		(at -18.41 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H36" smd circle
		(at -19.68 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H37" smd circle
		(at -20.95 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H38" smd circle
		(at -22.22 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H39" smd circle
		(at -23.49 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(pad "H40" smd circle
		(at -24.76 -3.22)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.227)
		(solder_paste_margin 0.127)
	)
	(embedded_fonts no)
	(model "antmicro_asp_134603_01.glb"
		(offset
			(xyz 32.404 -81.753 -13.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
