(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ASP-134603-01_mounting_holes"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ASP-134603-01_mounting_holes"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ASP-134603-01_mounting_holes"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://suddendocs.samtec.com/prints/asp-134603-01-mkt.pdf?_gl=1*lo47tf*_ga*MzYxMTM5My4xNjYzOTI3MDkz*_ga_3KFNZC07WW*MTY2MzkyNzA5My4xLjEuMTY2MzkyNzY5My42MC4wLjA."
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Mezzanine Connector, Vita 57 XMC, Array, Female, 1.27 mm, 4 Rows, 160 Contacts, Surface Mount"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ASP-134603-01"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Samtec"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ASP-134603-01_mounting_holes_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "C1")
					(number "C1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "C2")
					(number "C2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "C3")
					(number "C3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "C4")
					(number "C4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "C5")
					(number "C5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "C6")
					(number "C6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "C7")
					(number "C7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "C8")
					(number "C8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "C9")
					(number "C9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "C10")
					(number "C10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "C11")
					(number "C11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "C12")
					(number "C12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "C13")
					(number "C13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "C14")
					(number "C14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "C15")
					(number "C15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "C16")
					(number "C16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "C17")
					(number "C17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "C18")
					(number "C18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "C19")
					(number "C19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "C20")
					(number "C20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "C21")
					(number "C21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "C22")
					(number "C22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "C23")
					(number "C23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "C24")
					(number "C24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "C25")
					(number "C25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "C26")
					(number "C26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "C27")
					(number "C27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "C28")
					(number "C28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "C29")
					(number "C29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "C30")
					(number "C30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "C31")
					(number "C31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "C32")
					(number "C32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "C33")
					(number "C33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "C34")
					(number "C34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "C35")
					(number "C35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "C36")
					(number "C36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "C37")
					(number "C37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "C38")
					(number "C38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "C39")
					(number "C39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "C40")
					(number "C40")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(name "D1")
					(number "D1")
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "D2")
					(number "D2")
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "D3")
					(number "D3")
				)
				(pin passive line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "D4")
					(number "D4")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 3.81)
					(name "D5")
					(number "D5")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "D6")
					(number "D6")
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 3.81)
					(name "D7")
					(number "D7")
				)
				(pin passive line
					(at 27.94 -17.78 180)
					(length 3.81)
					(name "D8")
					(number "D8")
				)
				(pin passive line
					(at 27.94 -20.32 180)
					(length 3.81)
					(name "D9")
					(number "D9")
				)
				(pin passive line
					(at 27.94 -22.86 180)
					(length 3.81)
					(name "D10")
					(number "D10")
				)
				(pin passive line
					(at 27.94 -25.4 180)
					(length 3.81)
					(name "D11")
					(number "D11")
				)
				(pin passive line
					(at 27.94 -27.94 180)
					(length 3.81)
					(name "D12")
					(number "D12")
				)
				(pin passive line
					(at 27.94 -30.48 180)
					(length 3.81)
					(name "D13")
					(number "D13")
				)
				(pin passive line
					(at 27.94 -33.02 180)
					(length 3.81)
					(name "D14")
					(number "D14")
				)
				(pin passive line
					(at 27.94 -35.56 180)
					(length 3.81)
					(name "D15")
					(number "D15")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 3.81)
					(name "D16")
					(number "D16")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(name "D17")
					(number "D17")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(name "D18")
					(number "D18")
				)
				(pin passive line
					(at 27.94 -45.72 180)
					(length 3.81)
					(name "D19")
					(number "D19")
				)
				(pin passive line
					(at 27.94 -48.26 180)
					(length 3.81)
					(name "D20")
					(number "D20")
				)
				(pin passive line
					(at 27.94 -50.8 180)
					(length 3.81)
					(name "D21")
					(number "D21")
				)
				(pin passive line
					(at 27.94 -53.34 180)
					(length 3.81)
					(name "D22")
					(number "D22")
				)
				(pin passive line
					(at 27.94 -55.88 180)
					(length 3.81)
					(name "D23")
					(number "D23")
				)
				(pin passive line
					(at 27.94 -58.42 180)
					(length 3.81)
					(name "D24")
					(number "D24")
				)
				(pin passive line
					(at 27.94 -60.96 180)
					(length 3.81)
					(name "D25")
					(number "D25")
				)
				(pin passive line
					(at 27.94 -63.5 180)
					(length 3.81)
					(name "D26")
					(number "D26")
				)
				(pin passive line
					(at 27.94 -66.04 180)
					(length 3.81)
					(name "D27")
					(number "D27")
				)
				(pin passive line
					(at 27.94 -68.58 180)
					(length 3.81)
					(name "D28")
					(number "D28")
				)
				(pin passive line
					(at 27.94 -71.12 180)
					(length 3.81)
					(name "D29")
					(number "D29")
				)
				(pin passive line
					(at 27.94 -73.66 180)
					(length 3.81)
					(name "D30")
					(number "D30")
				)
				(pin passive line
					(at 27.94 -76.2 180)
					(length 3.81)
					(name "D31")
					(number "D31")
				)
				(pin passive line
					(at 27.94 -78.74 180)
					(length 3.81)
					(name "D32")
					(number "D32")
				)
				(pin passive line
					(at 27.94 -81.28 180)
					(length 3.81)
					(name "D33")
					(number "D33")
				)
				(pin passive line
					(at 27.94 -83.82 180)
					(length 3.81)
					(name "D34")
					(number "D34")
				)
				(pin passive line
					(at 27.94 -86.36 180)
					(length 3.81)
					(name "D35")
					(number "D35")
				)
				(pin passive line
					(at 27.94 -88.9 180)
					(length 3.81)
					(name "D36")
					(number "D36")
				)
				(pin passive line
					(at 27.94 -91.44 180)
					(length 3.81)
					(name "D37")
					(number "D37")
				)
				(pin passive line
					(at 27.94 -93.98 180)
					(length 3.81)
					(name "D38")
					(number "D38")
				)
				(pin passive line
					(at 27.94 -96.52 180)
					(length 3.81)
					(name "D39")
					(number "D39")
				)
				(pin passive line
					(at 27.94 -99.06 180)
					(length 3.81)
					(name "D40")
					(number "D40")
				)
			)
			(symbol "ASP-134603-01_mounting_holes_2_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "G1")
					(number "G1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "G2")
					(number "G2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "G3")
					(number "G3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "G4")
					(number "G4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "G5")
					(number "G5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "G6")
					(number "G6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "G7")
					(number "G7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "G8")
					(number "G8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "G9")
					(number "G9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "G10")
					(number "G10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "G11")
					(number "G11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "G12")
					(number "G12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "G13")
					(number "G13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "G14")
					(number "G14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "G15")
					(number "G15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "G16")
					(number "G16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "G17")
					(number "G17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "G18")
					(number "G18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "G19")
					(number "G19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "G20")
					(number "G20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "G21")
					(number "G21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "G22")
					(number "G22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "G23")
					(number "G23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "G24")
					(number "G24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "G25")
					(number "G25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "G26")
					(number "G26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "G27")
					(number "G27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "G28")
					(number "G28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "G29")
					(number "G29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "G30")
					(number "G30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "G31")
					(number "G31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "G32")
					(number "G32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "G33")
					(number "G33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "G34")
					(number "G34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "G35")
					(number "G35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "G36")
					(number "G36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "G37")
					(number "G37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "G38")
					(number "G38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "G39")
					(number "G39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "G40")
					(number "G40")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(name "H1")
					(number "H1")
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "H2")
					(number "H2")
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "H3")
					(number "H3")
				)
				(pin passive line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "H4")
					(number "H4")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 3.81)
					(name "H5")
					(number "H5")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "H6")
					(number "H6")
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 3.81)
					(name "H7")
					(number "H7")
				)
				(pin passive line
					(at 27.94 -17.78 180)
					(length 3.81)
					(name "H8")
					(number "H8")
				)
				(pin passive line
					(at 27.94 -20.32 180)
					(length 3.81)
					(name "H9")
					(number "H9")
				)
				(pin passive line
					(at 27.94 -22.86 180)
					(length 3.81)
					(name "H10")
					(number "H10")
				)
				(pin passive line
					(at 27.94 -25.4 180)
					(length 3.81)
					(name "H11")
					(number "H11")
				)
				(pin passive line
					(at 27.94 -27.94 180)
					(length 3.81)
					(name "H12")
					(number "H12")
				)
				(pin passive line
					(at 27.94 -30.48 180)
					(length 3.81)
					(name "H13")
					(number "H13")
				)
				(pin passive line
					(at 27.94 -33.02 180)
					(length 3.81)
					(name "H14")
					(number "H14")
				)
				(pin passive line
					(at 27.94 -35.56 180)
					(length 3.81)
					(name "H15")
					(number "H15")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 3.81)
					(name "H16")
					(number "H16")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(name "H17")
					(number "H17")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(name "H18")
					(number "H18")
				)
				(pin passive line
					(at 27.94 -45.72 180)
					(length 3.81)
					(name "H19")
					(number "H19")
				)
				(pin passive line
					(at 27.94 -48.26 180)
					(length 3.81)
					(name "H20")
					(number "H20")
				)
				(pin passive line
					(at 27.94 -50.8 180)
					(length 3.81)
					(name "H21")
					(number "H21")
				)
				(pin passive line
					(at 27.94 -53.34 180)
					(length 3.81)
					(name "H22")
					(number "H22")
				)
				(pin passive line
					(at 27.94 -55.88 180)
					(length 3.81)
					(name "H23")
					(number "H23")
				)
				(pin passive line
					(at 27.94 -58.42 180)
					(length 3.81)
					(name "H24")
					(number "H24")
				)
				(pin passive line
					(at 27.94 -60.96 180)
					(length 3.81)
					(name "H25")
					(number "H25")
				)
				(pin passive line
					(at 27.94 -63.5 180)
					(length 3.81)
					(name "H26")
					(number "H26")
				)
				(pin passive line
					(at 27.94 -66.04 180)
					(length 3.81)
					(name "H27")
					(number "H27")
				)
				(pin passive line
					(at 27.94 -68.58 180)
					(length 3.81)
					(name "H28")
					(number "H28")
				)
				(pin passive line
					(at 27.94 -71.12 180)
					(length 3.81)
					(name "H29")
					(number "H29")
				)
				(pin passive line
					(at 27.94 -73.66 180)
					(length 3.81)
					(name "H30")
					(number "H30")
				)
				(pin passive line
					(at 27.94 -76.2 180)
					(length 3.81)
					(name "H31")
					(number "H31")
				)
				(pin passive line
					(at 27.94 -78.74 180)
					(length 3.81)
					(name "H32")
					(number "H32")
				)
				(pin passive line
					(at 27.94 -81.28 180)
					(length 3.81)
					(name "H33")
					(number "H33")
				)
				(pin passive line
					(at 27.94 -83.82 180)
					(length 3.81)
					(name "H34")
					(number "H34")
				)
				(pin passive line
					(at 27.94 -86.36 180)
					(length 3.81)
					(name "H35")
					(number "H35")
				)
				(pin passive line
					(at 27.94 -88.9 180)
					(length 3.81)
					(name "H36")
					(number "H36")
				)
				(pin passive line
					(at 27.94 -91.44 180)
					(length 3.81)
					(name "H37")
					(number "H37")
				)
				(pin passive line
					(at 27.94 -93.98 180)
					(length 3.81)
					(name "H38")
					(number "H38")
				)
				(pin passive line
					(at 27.94 -96.52 180)
					(length 3.81)
					(name "H39")
					(number "H39")
				)
				(pin passive line
					(at 27.94 -99.06 180)
					(length 3.81)
					(name "H40")
					(number "H40")
				)
			)
			(embedded_fonts no)
		)
)
