(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ASP-184329-01"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 58.42 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ASP-184329-01"
				(at 58.42 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ASP-184329-01"
				(at 58.42 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/527/asp_184329_01_mkt-2854128.pdf"
				(at 58.42 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Mezzanine Connector, Array, Female, 1.27 mm, 14 Rows, 560 Contacts, Surface Mount"
				(at 58.42 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Samtec"
				(at 58.42 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ASP-184329-01"
				(at 58.42 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 58.42 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ASP-184329-01_1_1"
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "RES1")
					(number "L01")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L02")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L03")
				)
				(pin passive line
					(at 36.83 -11.43 180)
					(length 3.81)
					(name "GBTCLK4_M2C_P")
					(number "L04")
				)
				(pin passive line
					(at 36.83 -13.97 180)
					(length 3.81)
					(name "GBTCLK4_M2C_N")
					(number "L05")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L06")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L07")
				)
				(pin passive line
					(at 36.83 -16.51 180)
					(length 3.81)
					(name "GBTCLK3_M2C_P")
					(number "L08")
				)
				(pin passive line
					(at 36.83 -19.05 180)
					(length 3.81)
					(name "GBTCLK3_M2C_N")
					(number "L09")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 36.83 -21.59 180)
					(length 3.81)
					(name "GBTCLK2_M2C_P")
					(number "L12")
				)
				(pin passive line
					(at 36.83 -24.13 180)
					(length 3.81)
					(name "GBTCLK2_M2C_N")
					(number "L13")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L15")
				)
				(pin passive line
					(at 36.83 -26.67 180)
					(length 3.81)
					(name "SYNC_C2M_P")
					(number "L16")
				)
				(pin passive line
					(at 36.83 -29.21 180)
					(length 3.81)
					(name "SYNC_C2M_N")
					(number "L17")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L18")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L19")
				)
				(pin passive line
					(at 36.83 -31.75 180)
					(length 3.81)
					(name "REFCLK_C2M_P")
					(number "L20")
				)
				(pin passive line
					(at 36.83 -34.29 180)
					(length 3.81)
					(name "REFCLK_C2M_N")
					(number "L21")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L23")
				)
				(pin passive line
					(at 36.83 -36.83 180)
					(length 3.81)
					(name "REFCLK_M2C_P")
					(number "L24")
				)
				(pin passive line
					(at 36.83 -39.37 180)
					(length 3.81)
					(name "REFCLK_M2C_N")
					(number "L25")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L26")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L27")
				)
				(pin passive line
					(at 36.83 -41.91 180)
					(length 3.81)
					(name "SYNC_M2C_P")
					(number "L28")
				)
				(pin passive line
					(at 36.83 -44.45 180)
					(length 3.81)
					(name "SYNC_M2C_N")
					(number "L29")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L30")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L31")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "RES2")
					(number "L32")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 3.81)
					(name "RES3")
					(number "L33")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L34")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L35")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "12P0V")
					(number "L36")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "12P0V")
					(number "L37")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L38")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "L39")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "12P0V")
					(number "L40")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M01")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DP23_M2C_P")
					(number "M02")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DP23_M2C_N")
					(number "M03")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M04")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M05")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DP22_M2C_P")
					(number "M06")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DP22_M2C_N")
					(number "M07")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M08")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M09")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DP21_M2C_P")
					(number "M10")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DP21_M2C_N")
					(number "M11")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DP20_M2C_P")
					(number "M14")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DP20_M2C_N")
					(number "M15")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M16")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M17")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DP14_C2M_P")
					(number "M18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DP14_C2M_N")
					(number "M19")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M20")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DP15_C2M_P")
					(number "M22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DP15_C2M_N")
					(number "M23")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M24")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DP16_C2M_P")
					(number "M26")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DP16_C2M_N")
					(number "M27")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M28")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M29")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DP17_C2M_P")
					(number "M30")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DP17_C2M_N")
					(number "M31")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M32")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M33")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DP18_C2M_P")
					(number "M34")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DP18_C2M_N")
					(number "M35")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M36")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M37")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DP19_C2M_P")
					(number "M38")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DP19_C2M_N")
					(number "M39")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "GND")
					(number "M40")
				)
			)
			(symbol "ASP-184329-01_2_1"
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J01")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "CLK3_BIDIR_P")
					(number "J02")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "CLK3_BIDIR_N")
					(number "J03")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J04")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J05")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "HA03_P")
					(number "J06")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "HA03_N")
					(number "J07")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J08")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "HA07_P")
					(number "J09")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "HA07_N")
					(number "J10")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "HA11_P")
					(number "J12")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "HA11_N")
					(number "J13")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "HA14_P")
					(number "J15")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "HA14_N")
					(number "J16")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J17")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "HA18_P")
					(number "J18")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "HA18_N")
					(number "J19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "HA22_P")
					(number "J21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "HA22_N")
					(number "J22")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J23")
				)
				(pin passive line
					(at 36.83 -16.51 180)
					(length 3.81)
					(name "HB01_P")
					(number "J24")
				)
				(pin passive line
					(at 36.83 -19.05 180)
					(length 3.81)
					(name "HB01_N")
					(number "J25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J26")
				)
				(pin passive line
					(at 36.83 -26.67 180)
					(length 3.81)
					(name "HB07_P")
					(number "J27")
				)
				(pin passive line
					(at 36.83 -29.21 180)
					(length 3.81)
					(name "HB07_N")
					(number "J28")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J29")
				)
				(pin passive line
					(at 36.83 -36.83 180)
					(length 3.81)
					(name "HB11_P")
					(number "J30")
				)
				(pin passive line
					(at 36.83 -39.37 180)
					(length 3.81)
					(name "HB11_N")
					(number "J31")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J32")
				)
				(pin passive line
					(at 36.83 -46.99 180)
					(length 3.81)
					(name "HB15_P")
					(number "J33")
				)
				(pin passive line
					(at 36.83 -49.53 180)
					(length 3.81)
					(name "HB15_N")
					(number "J34")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J35")
				)
				(pin passive line
					(at 36.83 -57.15 180)
					(length 3.81)
					(name "HB18_P")
					(number "J36")
				)
				(pin passive line
					(at 36.83 -59.69 180)
					(length 3.81)
					(name "HB18_N")
					(number "J37")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J38")
				)
				(pin passive line
					(at 36.83 -66.04 180)
					(length 3.81)
					(name "VIO_B_M2C")
					(number "J39")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "J40")
				)
				(pin passive line
					(at 36.83 -63.5 180)
					(length 3.81)
					(name "VREF_B_M2C")
					(number "K01")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K02")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K03")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "CLK2_BIDIR_P")
					(number "K04")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 3.81)
					(name "CLK2_BIDIR_N")
					(number "K05")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K06")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "HA02_P")
					(number "K07")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "HA02_N")
					(number "K08")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K09")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "HA06_P")
					(number "K10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "HA06_N")
					(number "K11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K12")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "HA10_P")
					(number "K13")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "HA10_N")
					(number "K14")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K15")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "HA17_P_CC")
					(number "K16")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "HA17_N_CC")
					(number "K17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "HA21_P")
					(number "K19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "HA21_N")
					(number "K20")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K21")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "HA23_P")
					(number "K22")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "HA23_N")
					(number "K23")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K24")
				)
				(pin passive line
					(at 36.83 -11.43 180)
					(length 3.81)
					(name "HB00_P_CC")
					(number "K25")
				)
				(pin passive line
					(at 36.83 -13.97 180)
					(length 3.81)
					(name "HB00_N_CC")
					(number "K26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K27")
				)
				(pin passive line
					(at 36.83 -21.59 180)
					(length 3.81)
					(name "HB06_P_CC")
					(number "K28")
				)
				(pin passive line
					(at 36.83 -24.13 180)
					(length 3.81)
					(name "HB06_N_CC")
					(number "K29")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K30")
				)
				(pin passive line
					(at 36.83 -31.75 180)
					(length 3.81)
					(name "HB10_P")
					(number "K31")
				)
				(pin passive line
					(at 36.83 -34.29 180)
					(length 3.81)
					(name "HB10_N")
					(number "K32")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K33")
				)
				(pin passive line
					(at 36.83 -41.91 180)
					(length 3.81)
					(name "HB14_P")
					(number "K34")
				)
				(pin passive line
					(at 36.83 -44.45 180)
					(length 3.81)
					(name "HB14_N")
					(number "K35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K36")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "HB17_P_CC")
					(number "K37")
				)
				(pin passive line
					(at 36.83 -54.61 180)
					(length 3.81)
					(name "HB17_N_CC")
					(number "K38")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GND")
					(number "K39")
				)
				(pin passive line
					(at 36.83 -66.04 180)
					(length 3.81)
					(name "VIO_B_M2C")
					(number "K40")
				)
			)
			(symbol "ASP-184329-01_3_1"
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G01")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "CLK1_M2C_P")
					(number "G02")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "CLK1_M2C_N")
					(number "G03")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G04")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G05")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "LA00_P_CC")
					(number "G06")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "LA00_N_CC")
					(number "G07")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G08")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "LA03_P")
					(number "G09")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "LA03_N")
					(number "G10")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "LA08_P")
					(number "G12")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "LA08_N")
					(number "G13")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LA12_P")
					(number "G15")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "LA12_N")
					(number "G16")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G17")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "LA16_P")
					(number "G18")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "LA16_N")
					(number "G19")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G20")
				)
				(pin passive line
					(at 36.83 -10.16 180)
					(length 3.81)
					(name "LA20_P")
					(number "G21")
				)
				(pin passive line
					(at 36.83 -12.7 180)
					(length 3.81)
					(name "LA20_N")
					(number "G22")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G23")
				)
				(pin passive line
					(at 36.83 -20.32 180)
					(length 3.81)
					(name "LA22_P")
					(number "G24")
				)
				(pin passive line
					(at 36.83 -22.86 180)
					(length 3.81)
					(name "LA22_N")
					(number "G25")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G26")
				)
				(pin passive line
					(at 36.83 -30.48 180)
					(length 3.81)
					(name "LA25_P")
					(number "G27")
				)
				(pin passive line
					(at 36.83 -33.02 180)
					(length 3.81)
					(name "LA25_N")
					(number "G28")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G29")
				)
				(pin passive line
					(at 36.83 -40.64 180)
					(length 3.81)
					(name "LA29_P")
					(number "G30")
				)
				(pin passive line
					(at 36.83 -43.18 180)
					(length 3.81)
					(name "LA29_N")
					(number "G31")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G32")
				)
				(pin passive line
					(at 36.83 -50.8 180)
					(length 3.81)
					(name "LA31_P")
					(number "G33")
				)
				(pin passive line
					(at 36.83 -53.34 180)
					(length 3.81)
					(name "LA31_N")
					(number "G34")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G35")
				)
				(pin passive line
					(at 36.83 -60.96 180)
					(length 3.81)
					(name "LA33_P")
					(number "G36")
				)
				(pin passive line
					(at 36.83 -63.5 180)
					(length 3.81)
					(name "LA33_N")
					(number "G37")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G38")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VADJ")
					(number "G39")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "G40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VREF_A_M2C")
					(number "H01")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PRSNT_M2C_L")
					(number "H02")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H03")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CLK0_M2C_P")
					(number "H04")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(name "CLK0_M2C_N")
					(number "H05")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H06")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "LA02_P")
					(number "H07")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "LA02_N")
					(number "H08")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H09")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "LA04_P")
					(number "H10")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "LA04_N")
					(number "H11")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "LA07_P")
					(number "H13")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "LA07_N")
					(number "H14")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H15")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LA11_P")
					(number "H16")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "LA11_N")
					(number "H17")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "LA15_P")
					(number "H19")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "LA15_N")
					(number "H20")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H21")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "LA19_P")
					(number "H22")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 3.81)
					(name "LA19_N")
					(number "H23")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H24")
				)
				(pin passive line
					(at 36.83 -15.24 180)
					(length 3.81)
					(name "LA21_P")
					(number "H25")
				)
				(pin passive line
					(at 36.83 -17.78 180)
					(length 3.81)
					(name "LA21_N")
					(number "H26")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H27")
				)
				(pin passive line
					(at 36.83 -25.4 180)
					(length 3.81)
					(name "LA24_P")
					(number "H28")
				)
				(pin passive line
					(at 36.83 -27.94 180)
					(length 3.81)
					(name "LA24_N")
					(number "H29")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H30")
				)
				(pin passive line
					(at 36.83 -35.56 180)
					(length 3.81)
					(name "LA28_P")
					(number "H31")
				)
				(pin passive line
					(at 36.83 -38.1 180)
					(length 3.81)
					(name "LA28_N")
					(number "H32")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H33")
				)
				(pin passive line
					(at 36.83 -45.72 180)
					(length 3.81)
					(name "LA30_P")
					(number "H34")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "LA30_N")
					(number "H35")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H36")
				)
				(pin passive line
					(at 36.83 -55.88 180)
					(length 3.81)
					(name "LA32_P")
					(number "H37")
				)
				(pin passive line
					(at 36.83 -58.42 180)
					(length 3.81)
					(name "LA32_N")
					(number "H38")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 3.81)
					(name "GND")
					(number "H39")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VADJ")
					(number "H40")
				)
			)
			(symbol "ASP-184329-01_4_1"
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E01")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(name "HA01_P_CC")
					(number "E02")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "HA01_N_CC")
					(number "E03")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E04")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E05")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "HA05_P")
					(number "E06")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "HA05_N")
					(number "E07")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E08")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "HA09_P")
					(number "E09")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "HA09_N")
					(number "E10")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "HA13_P")
					(number "E12")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "HA13_N")
					(number "E13")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E14")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "HA16_P")
					(number "E15")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 3.81)
					(name "HA16_N")
					(number "E16")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E17")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "HA20_P")
					(number "E18")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 3.81)
					(name "HA20_N")
					(number "E19")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E20")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "HB03_P")
					(number "E21")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 3.81)
					(name "HB03_N")
					(number "E22")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E23")
				)
				(pin passive line
					(at 36.83 -15.24 180)
					(length 3.81)
					(name "HB05_P")
					(number "E24")
				)
				(pin passive line
					(at 36.83 -17.78 180)
					(length 3.81)
					(name "HB05_N")
					(number "E25")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E26")
				)
				(pin passive line
					(at 36.83 -25.4 180)
					(length 3.81)
					(name "HB09_P")
					(number "E27")
				)
				(pin passive line
					(at 36.83 -27.94 180)
					(length 3.81)
					(name "HB09_N")
					(number "E28")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E29")
				)
				(pin passive line
					(at 36.83 -35.56 180)
					(length 3.81)
					(name "HB13_P")
					(number "E30")
				)
				(pin passive line
					(at 36.83 -38.1 180)
					(length 3.81)
					(name "HB13_N")
					(number "E31")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E32")
				)
				(pin passive line
					(at 36.83 -45.72 180)
					(length 3.81)
					(name "HB19_P")
					(number "E33")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "HB19_N")
					(number "E34")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E35")
				)
				(pin passive line
					(at 36.83 -55.88 180)
					(length 3.81)
					(name "HB21_P")
					(number "E36")
				)
				(pin passive line
					(at 36.83 -58.42 180)
					(length 3.81)
					(name "HB21_N")
					(number "E37")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E38")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VADJ")
					(number "E39")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "E40")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "PG_M2C")
					(number "F01")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F02")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F03")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "HA00_P_CC")
					(number "F04")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "HA00_N_CC")
					(number "F05")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F06")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "HA04_P")
					(number "F07")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "HA04_N")
					(number "F08")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F09")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "HA08_P")
					(number "F10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "HA08_N")
					(number "F11")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "HA12_P")
					(number "F13")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "HA12_N")
					(number "F14")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F15")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "HA15_P")
					(number "F16")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "HA15_N")
					(number "F17")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F18")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "HA19_P")
					(number "F19")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "HA19_N")
					(number "F20")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F21")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "HB02_P")
					(number "F22")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "HB02_N")
					(number "F23")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F24")
				)
				(pin passive line
					(at 36.83 -10.16 180)
					(length 3.81)
					(name "HB04_P")
					(number "F25")
				)
				(pin passive line
					(at 36.83 -12.7 180)
					(length 3.81)
					(name "HB04_N")
					(number "F26")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F27")
				)
				(pin passive line
					(at 36.83 -20.32 180)
					(length 3.81)
					(name "HB08_P")
					(number "F28")
				)
				(pin passive line
					(at 36.83 -22.86 180)
					(length 3.81)
					(name "HB08_N")
					(number "F29")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F30")
				)
				(pin passive line
					(at 36.83 -30.48 180)
					(length 3.81)
					(name "HB12_P")
					(number "F31")
				)
				(pin passive line
					(at 36.83 -33.02 180)
					(length 3.81)
					(name "HB12_N")
					(number "F32")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F33")
				)
				(pin passive line
					(at 36.83 -40.64 180)
					(length 3.81)
					(name "HB16_P")
					(number "F34")
				)
				(pin passive line
					(at 36.83 -43.18 180)
					(length 3.81)
					(name "HB16_N")
					(number "F35")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F36")
				)
				(pin passive line
					(at 36.83 -50.8 180)
					(length 3.81)
					(name "HB20_P")
					(number "F37")
				)
				(pin passive line
					(at 36.83 -53.34 180)
					(length 3.81)
					(name "HB20_N")
					(number "F38")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 3.81)
					(name "GND")
					(number "F39")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VADJ")
					(number "F40")
				)
			)
			(symbol "ASP-184329-01_5_1"
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C01")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DP0_C2M_P")
					(number "C02")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DP0_C2M_N")
					(number "C03")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C04")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C05")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DP0_M2C_P")
					(number "C06")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DP0_M2C_N")
					(number "C07")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C08")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C09")
				)
				(pin passive line
					(at 36.83 -10.16 180)
					(length 3.81)
					(name "LA06_P")
					(number "C10")
				)
				(pin passive line
					(at 36.83 -12.7 180)
					(length 3.81)
					(name "LA06_N")
					(number "C11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C13")
				)
				(pin passive line
					(at 36.83 -20.32 180)
					(length 3.81)
					(name "LA10_P")
					(number "C14")
				)
				(pin passive line
					(at 36.83 -22.86 180)
					(length 3.81)
					(name "LA10_N")
					(number "C15")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C16")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C17")
				)
				(pin passive line
					(at 36.83 -30.48 180)
					(length 3.81)
					(name "LA14_P")
					(number "C18")
				)
				(pin passive line
					(at 36.83 -33.02 180)
					(length 3.81)
					(name "LA14_N")
					(number "C19")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C20")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C21")
				)
				(pin passive line
					(at 36.83 -40.64 180)
					(length 3.81)
					(name "LA18_P_CC")
					(number "C22")
				)
				(pin passive line
					(at 36.83 -43.18 180)
					(length 3.81)
					(name "LA18_N_CC")
					(number "C23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C24")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C25")
				)
				(pin passive line
					(at 36.83 -55.88 180)
					(length 3.81)
					(name "LA27_P")
					(number "C26")
				)
				(pin passive line
					(at 36.83 -58.42 180)
					(length 3.81)
					(name "LA27_N")
					(number "C27")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C28")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C29")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "SCL")
					(number "C30")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SDA")
					(number "C31")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C32")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C33")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(name "GA0")
					(number "C34")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "12P0V")
					(number "C35")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C36")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "12P0V")
					(number "C37")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C38")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3P3V")
					(number "C39")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "C40")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "PG_C2M")
					(number "D01")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D02")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D03")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "GBTCLK0_M2C_P")
					(number "D04")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "GBTCLK0_M2C_N")
					(number "D05")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D06")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D07")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "LA01_P_CC")
					(number "D08")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "LA01_N_CC")
					(number "D09")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D10")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "LA05_P")
					(number "D11")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 3.81)
					(name "LA05_N")
					(number "D12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 36.83 -15.24 180)
					(length 3.81)
					(name "LA09_P")
					(number "D14")
				)
				(pin passive line
					(at 36.83 -17.78 180)
					(length 3.81)
					(name "LA09_N")
					(number "D15")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D16")
				)
				(pin passive line
					(at 36.83 -25.4 180)
					(length 3.81)
					(name "LA13_P")
					(number "D17")
				)
				(pin passive line
					(at 36.83 -27.94 180)
					(length 3.81)
					(name "LA13_N")
					(number "D18")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D19")
				)
				(pin passive line
					(at 36.83 -35.56 180)
					(length 3.81)
					(name "LA17_P_CC")
					(number "D20")
				)
				(pin passive line
					(at 36.83 -38.1 180)
					(length 3.81)
					(name "LA17_N_CC")
					(number "D21")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D22")
				)
				(pin passive line
					(at 36.83 -45.72 180)
					(length 3.81)
					(name "LA23_P")
					(number "D23")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "LA23_N")
					(number "D24")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D25")
				)
				(pin passive line
					(at 36.83 -50.8 180)
					(length 3.81)
					(name "LA26_P")
					(number "D26")
				)
				(pin passive line
					(at 36.83 -53.34 180)
					(length 3.81)
					(name "LA26_N")
					(number "D27")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D28")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "TCK")
					(number "D29")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "TDI")
					(number "D30")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "TDO")
					(number "D31")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "3P3VAUX")
					(number "D32")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "TMS")
					(number "D33")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "TRST_L")
					(number "D34")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "GA1")
					(number "D35")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3P3V")
					(number "D36")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D37")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3P3V")
					(number "D38")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GND")
					(number "D39")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3P3V")
					(number "D40")
				)
			)
			(symbol "ASP-184329-01_6_1"
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A01")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DP1_M2C_P")
					(number "A02")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DP1_M2C_N")
					(number "A03")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A04")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A05")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DP2_M2C_P")
					(number "A06")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DP2_M2C_N")
					(number "A07")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A08")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A09")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DP3_M2C_P")
					(number "A10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DP3_M2C_N")
					(number "A11")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A13")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DP4_M2C_P")
					(number "A14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DP4_M2C_N")
					(number "A15")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A16")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A17")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DP5_M2C_P")
					(number "A18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DP5_M2C_N")
					(number "A19")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DP1_C2M_P")
					(number "A22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DP1_C2M_N")
					(number "A23")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A24")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A25")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DP2_C2M_P")
					(number "A26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DP2_C2M_N")
					(number "A27")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A28")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A29")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DP3_C2M_P")
					(number "A30")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DP3_C2M_N")
					(number "A31")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A33")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DP4_C2M_P")
					(number "A34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DP4_C2M_N")
					(number "A35")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A36")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A37")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DP5_C2M_P")
					(number "A38")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DP5_C2M_N")
					(number "A39")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "A40")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "CLK_DIR")
					(number "B01")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B02")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B03")
				)
				(pin passive line
					(at 36.83 -48.26 180)
					(length 3.81)
					(name "DP9_M2C_P")
					(number "B04")
				)
				(pin passive line
					(at 36.83 -50.8 180)
					(length 3.81)
					(name "DP9_M2C_N")
					(number "B05")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B06")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B07")
				)
				(pin passive line
					(at 36.83 -43.18 180)
					(length 3.81)
					(name "DP8_M2C_P")
					(number "B08")
				)
				(pin passive line
					(at 36.83 -45.72 180)
					(length 3.81)
					(name "DP8_M2C_N")
					(number "B09")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B10")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 36.83 -38.1 180)
					(length 3.81)
					(name "DP7_M2C_P")
					(number "B12")
				)
				(pin passive line
					(at 36.83 -40.64 180)
					(length 3.81)
					(name "DP7_M2C_N")
					(number "B13")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B14")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B15")
				)
				(pin passive line
					(at 36.83 -33.02 180)
					(length 3.81)
					(name "DP6_M2C_P")
					(number "B16")
				)
				(pin passive line
					(at 36.83 -35.56 180)
					(length 3.81)
					(name "DP6_M2C_N")
					(number "B17")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B18")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B19")
				)
				(pin passive line
					(at 36.83 -6.35 180)
					(length 3.81)
					(name "GBTCLK1_M2C_P")
					(number "B20")
				)
				(pin passive line
					(at 36.83 -8.89 180)
					(length 3.81)
					(name "GBTCLK1_M2C_N")
					(number "B21")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B23")
				)
				(pin passive line
					(at 36.83 -27.94 180)
					(length 3.81)
					(name "DP9_C2M_P")
					(number "B24")
				)
				(pin passive line
					(at 36.83 -30.48 180)
					(length 3.81)
					(name "DP9_C2M_N")
					(number "B25")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B26")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B27")
				)
				(pin passive line
					(at 36.83 -22.86 180)
					(length 3.81)
					(name "DP8_C2M_P")
					(number "B28")
				)
				(pin passive line
					(at 36.83 -25.4 180)
					(length 3.81)
					(name "DP8_C2M_N")
					(number "B29")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B30")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B31")
				)
				(pin passive line
					(at 36.83 -17.78 180)
					(length 3.81)
					(name "DP7_C2M_P")
					(number "B32")
				)
				(pin passive line
					(at 36.83 -20.32 180)
					(length 3.81)
					(name "DP7_C2M_N")
					(number "B33")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B34")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B35")
				)
				(pin passive line
					(at 36.83 -12.7 180)
					(length 3.81)
					(name "DP6_C2M_P")
					(number "B36")
				)
				(pin passive line
					(at 36.83 -15.24 180)
					(length 3.81)
					(name "DP6_C2M_N")
					(number "B37")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B38")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GND")
					(number "B39")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "RES0")
					(number "B40")
				)
			)
			(symbol "ASP-184329-01_7_1"
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y01")
				)
				(pin passive line
					(at 36.83 -44.45 180)
					(length 3.81)
					(name "DP23_C2M_P")
					(number "Y02")
				)
				(pin passive line
					(at 36.83 -46.99 180)
					(length 3.81)
					(name "DP23_C2M_N")
					(number "Y03")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y04")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y05")
				)
				(pin passive line
					(at 36.83 -34.29 180)
					(length 3.81)
					(name "DP21_C2M_P")
					(number "Y06")
				)
				(pin passive line
					(at 36.83 -36.83 180)
					(length 3.81)
					(name "DP21_C2M_N")
					(number "Y07")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y08")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y09")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 3.81)
					(name "DP10_M2C_P")
					(number "Y10")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "DP10_M2C_N")
					(number "Y11")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y12")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y13")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "DP12_M2C_P")
					(number "Y14")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "DP12_M2C_N")
					(number "Y15")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y16")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y17")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "DP14_M2C_P")
					(number "Y18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "DP14_M2C_N")
					(number "Y19")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y20")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y21")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "DP15_M2C_P")
					(number "Y22")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "DP15_M2C_N")
					(number "Y23")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y24")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y25")
				)
				(pin passive line
					(at 36.83 -13.97 180)
					(length 3.81)
					(name "DP11_C2M_P")
					(number "Y26")
				)
				(pin passive line
					(at 36.83 -16.51 180)
					(length 3.81)
					(name "DP11_C2M_N")
					(number "Y27")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y28")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y29")
				)
				(pin passive line
					(at 36.83 -24.13 180)
					(length 3.81)
					(name "DP13_C2M_P")
					(number "Y30")
				)
				(pin passive line
					(at 36.83 -26.67 180)
					(length 3.81)
					(name "DP13_C2M_N")
					(number "Y31")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y32")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y33")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "DP17_M2C_P")
					(number "Y34")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "DP17_M2C_N")
					(number "Y35")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y36")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y37")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "DP19_M2C_P")
					(number "Y38")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "DP19_M2C_N")
					(number "Y39")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Y40")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 3.81)
					(name "HSPC_PRSNT_M2C_L")
					(number "Z01")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z02")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z03")
				)
				(pin passive line
					(at 36.83 -39.37 180)
					(length 3.81)
					(name "DP22_C2M_P")
					(number "Z04")
				)
				(pin passive line
					(at 36.83 -41.91 180)
					(length 3.81)
					(name "DP22_C2M_N")
					(number "Z05")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z06")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z07")
				)
				(pin passive line
					(at 36.83 -29.21 180)
					(length 3.81)
					(name "DP20_C2M_P")
					(number "Z08")
				)
				(pin passive line
					(at 36.83 -31.75 180)
					(length 3.81)
					(name "DP20_C2M_N")
					(number "Z09")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z10")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z11")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "DP11_M2C_P")
					(number "Z12")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(name "DP11_M2C_N")
					(number "Z13")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z14")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z15")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "DP13_M2C_P")
					(number "Z16")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "DP13_M2C_N")
					(number "Z17")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z18")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z19")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 3.81)
					(name "GBTCLK5_M2C_P")
					(number "Z20")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 3.81)
					(name "GBTCLK5_M2C_N")
					(number "Z21")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z22")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z23")
				)
				(pin passive line
					(at 36.83 -8.89 180)
					(length 3.81)
					(name "DP10_C2M_P")
					(number "Z24")
				)
				(pin passive line
					(at 36.83 -11.43 180)
					(length 3.81)
					(name "DP10_C2M_N")
					(number "Z25")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z26")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z27")
				)
				(pin passive line
					(at 36.83 -19.05 180)
					(length 3.81)
					(name "DP12_C2M_P")
					(number "Z28")
				)
				(pin passive line
					(at 36.83 -21.59 180)
					(length 3.81)
					(name "DP12_C2M_N")
					(number "Z29")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z30")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z31")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "DP16_M2C_P")
					(number "Z32")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "DP16_M2C_N")
					(number "Z33")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z34")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z35")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "DP18_M2C_P")
					(number "Z36")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "DP18_M2C_N")
					(number "Z37")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z38")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "Z39")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "3P3V")
					(number "Z40")
				)
			)
			(embedded_fonts no)
		)
)
