(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CBTL04083ABS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CBTL04083ABS"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CBTL04083ABS"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/CBTL04083A_CBTL04083B.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DisplayPort, PCIe, USB Switch IC 4 Channel 42-HVQFN (3.5x9)"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CBTL04083ABS"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PCIE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "HVQFN42_SOT1144-1_NXP HVQFN42_SOT1144-1_NXP-M HVQFN42_SOT1144-1_NXP-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CBTL04083ABS_1_1"
				(pin power_out line
					(at 0 -43.18 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A0_P")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A0_N")
					(number "3")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "A1_P")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "A1_N")
					(number "7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "8")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "SEL")
					(number "9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A2_P")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A2_N")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "13")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A3_P")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A3_N")
					(number "16")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "18")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "XSD23")
					(number "19")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "20")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "C3_N")
					(number "22")
				)
				(pin bidirectional line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "C3_P")
					(number "23")
				)
				(pin bidirectional line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "C2_N")
					(number "24")
				)
				(pin bidirectional line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "C2_P")
					(number "25")
				)
				(pin bidirectional line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "B3_N")
					(number "26")
				)
				(pin bidirectional line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "B3_P")
					(number "27")
				)
				(pin bidirectional line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "B2_N")
					(number "28")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "B2_P")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "30")
				)
				(pin bidirectional line
					(at 25.4 -21.59 180)
					(length 2.54)
					(name "C1_N")
					(number "31")
				)
				(pin bidirectional line
					(at 25.4 -19.05 180)
					(length 2.54)
					(name "C1_P")
					(number "32")
				)
				(pin bidirectional line
					(at 25.4 -16.51 180)
					(length 2.54)
					(name "C0_N")
					(number "33")
				)
				(pin bidirectional line
					(at 25.4 -13.97 180)
					(length 2.54)
					(name "C0_P")
					(number "34")
				)
				(pin bidirectional line
					(at 25.4 -11.43 180)
					(length 2.54)
					(name "B1_N")
					(number "35")
				)
				(pin bidirectional line
					(at 25.4 -8.89 180)
					(length 2.54)
					(name "B1_P")
					(number "36")
				)
				(pin bidirectional line
					(at 25.4 -6.35 180)
					(length 2.54)
					(name "B0_N")
					(number "37")
				)
				(pin bidirectional line
					(at 25.4 -3.81 180)
					(length 2.54)
					(name "B0_P")
					(number "38")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "40")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "XSD01")
					(number "41")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "42")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
			)
			(embedded_fonts no)
		)
)
