(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CP2103-GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CP2103-GM"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CP2103-GM"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/368/CP2103-1397886.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Controller Interface IC USB to UART Bridge QFN28"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CP2103-GM"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, INTERFACE, BRIDGE, SMT, USB, UART, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CP2103-GM_1_1"
				(pin input line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "RI")
					(number "1")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D+")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D-")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "VIO")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD")
					(number "6")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "REGIN")
					(number "7")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "VBUS")
					(number "8")
				)
				(pin bidirectional line
					(at 21.59 -10.16 180)
					(length 2.54)
					(name "~{RST}")
					(number "9")
				)
				(pin no_connect line
					(at 2.54 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin output line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "~{SUSPEND}")
					(number "11")
				)
				(pin output line
					(at 21.59 -15.24 180)
					(length 2.54)
					(name "SUSPEND")
					(number "12")
				)
				(pin no_connect line
					(at 2.54 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin no_connect line
					(at 2.54 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin bidirectional line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "GPIO.3")
					(number "16")
				)
				(pin bidirectional line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "GPIO.2")
					(number "17")
				)
				(pin bidirectional line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "GPIO.1")
					(number "18")
				)
				(pin bidirectional line
					(at 21.59 0 180)
					(length 2.54)
					(name "GPIO.0")
					(number "19")
				)
				(pin no_connect line
					(at 2.54 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin input line
					(at 21.59 -35.56 180)
					(length 2.54)
					(name "CTS")
					(number "22")
				)
				(pin output line
					(at 21.59 -33.02 180)
					(length 2.54)
					(name "RTS")
					(number "23")
				)
				(pin input line
					(at 21.59 -30.48 180)
					(length 2.54)
					(name "RXD")
					(number "24")
				)
				(pin output line
					(at 21.59 -27.94 180)
					(length 2.54)
					(name "TXD")
					(number "25")
				)
				(pin input line
					(at 21.59 -25.4 180)
					(length 2.54)
					(name "DSR")
					(number "26")
				)
				(pin output line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "DTR")
					(number "27")
				)
				(pin input line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "DCD")
					(number "28")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "EPAD")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
