(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CP2108-B02-GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CP2108-B02-GM"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CP2108-B02-GM"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/368/cp2108-datasheet-1509353.pdf"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB to Quad UART Bridge Controller 64-Pin QFN EP T/R"
				(at 63.5 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CP2108-B02-GM"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 63.5 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, USB, UART, CONVERTER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CP2108-B02-GM_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "RX3")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VSSHD")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VIOHD")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TX3")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CTS3")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RTS3")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RI3")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DCD3")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DSR3")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DTR3")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RI2")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DCD2")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "CTS2")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RTS2")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RX2")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "TX2")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DSR2")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "TSR2")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "~{SUSPEND_1}")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "~{SUSPEND_2}")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "GPIO.15")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "GPIO.14")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GPIO.13")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "VIO_1")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "VSS_1")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "GPIO.12")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "GPIO.11")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "GPIO.10")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GPIO.9")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "GPIO.8")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "GPIO.7")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "GPIO.6")
					(number "32")
				)
				(pin bidirectional line
					(at 50.8 0 180)
					(length 2.54)
					(name "GPIO.5")
					(number "33")
				)
				(pin bidirectional line
					(at 50.8 -2.54 180)
					(length 2.54)
					(name "GPIO.4")
					(number "34")
				)
				(pin no_connect line
					(at 48.26 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "35")
				)
				(pin no_connect line
					(at 48.26 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "36")
				)
				(pin bidirectional line
					(at 50.8 -10.16 180)
					(length 2.54)
					(name "GPIO.3")
					(number "37")
				)
				(pin bidirectional line
					(at 50.8 -12.7 180)
					(length 2.54)
					(name "GPIO.2")
					(number "38")
				)
				(pin bidirectional line
					(at 50.8 -15.24 180)
					(length 2.54)
					(name "VIO_2")
					(number "39")
				)
				(pin bidirectional line
					(at 50.8 -17.78 180)
					(length 2.54)
					(name "GPIO.1")
					(number "40")
				)
				(pin bidirectional line
					(at 50.8 -20.32 180)
					(length 2.54)
					(name "GPIO.0")
					(number "41")
				)
				(pin bidirectional line
					(at 50.8 -22.86 180)
					(length 2.54)
					(name "RI1")
					(number "42")
				)
				(pin bidirectional line
					(at 50.8 -25.4 180)
					(length 2.54)
					(name "DCD1")
					(number "43")
				)
				(pin bidirectional line
					(at 50.8 -27.94 180)
					(length 2.54)
					(name "DSR1")
					(number "44")
				)
				(pin bidirectional line
					(at 50.8 -30.48 180)
					(length 2.54)
					(name "DTR1")
					(number "45")
				)
				(pin bidirectional line
					(at 50.8 -33.02 180)
					(length 2.54)
					(name "CTS1")
					(number "46")
				)
				(pin bidirectional line
					(at 50.8 -35.56 180)
					(length 2.54)
					(name "RTS1")
					(number "47")
				)
				(pin bidirectional line
					(at 50.8 -38.1 180)
					(length 2.54)
					(name "RX1")
					(number "48")
				)
				(pin bidirectional line
					(at 50.8 -40.64 180)
					(length 2.54)
					(name "TX1")
					(number "49")
				)
				(pin bidirectional line
					(at 50.8 -43.18 180)
					(length 2.54)
					(name "RI0")
					(number "50")
				)
				(pin bidirectional line
					(at 50.8 -45.72 180)
					(length 2.54)
					(name "DCD0")
					(number "51")
				)
				(pin bidirectional line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "DSR0")
					(number "52")
				)
				(pin bidirectional line
					(at 50.8 -50.8 180)
					(length 2.54)
					(name "DTR0")
					(number "53")
				)
				(pin bidirectional line
					(at 50.8 -53.34 180)
					(length 2.54)
					(name "CTS0")
					(number "54")
				)
				(pin bidirectional line
					(at 50.8 -55.88 180)
					(length 2.54)
					(name "RTS0")
					(number "55")
				)
				(pin bidirectional line
					(at 50.8 -58.42 180)
					(length 2.54)
					(name "RX0")
					(number "56")
				)
				(pin bidirectional line
					(at 50.8 -60.96 180)
					(length 2.54)
					(name "TX0")
					(number "57")
				)
				(pin bidirectional line
					(at 50.8 -63.5 180)
					(length 2.54)
					(name "VDD")
					(number "58")
				)
				(pin bidirectional line
					(at 50.8 -66.04 180)
					(length 2.54)
					(name "VSS_2")
					(number "59")
				)
				(pin bidirectional line
					(at 50.8 -68.58 180)
					(length 2.54)
					(name "VREGIN")
					(number "60")
				)
				(pin bidirectional line
					(at 50.8 -71.12 180)
					(length 2.54)
					(name "VBUS")
					(number "61")
				)
				(pin bidirectional line
					(at 50.8 -73.66 180)
					(length 2.54)
					(name "D+")
					(number "62")
				)
				(pin bidirectional line
					(at 50.8 -76.2 180)
					(length 2.54)
					(name "D-")
					(number "63")
				)
				(pin bidirectional line
					(at 50.8 -78.74 180)
					(length 2.54)
					(name "~{RESET}")
					(number "64")
				)
				(pin bidirectional line
					(at 50.8 -81.28 180)
					(length 2.54)
					(name "VSS_(THERMAL_PAD)")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
