(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CY7C65219-40LQXIT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CY7C65219-40LQXIT"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CY7C65219-40LQXIT"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.in/datasheet/2/100/002-20954_CY7C65219_DOCK_MANAGEMENT_CONTROLLER_DMC-1276163.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB full-speed capability to support USB Billboard device"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CY7C65219-40LQXIT "
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CY7C65219-40LQXIT_1_1"
				(pin no_connect line
					(at 8.89 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin no_connect line
					(at 11.43 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 16.51 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 8.89 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 19.05 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 21.59 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P1.0")
					(number "7")
					(alternate "GPIO_1_0" passive line)
					(alternate "SPI_2_MISO" passive line)
					(alternate "UART_2_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "P1.1")
					(number "8")
					(alternate "GPIO_1_1" passive line)
					(alternate "SPI_2_SEL" passive line)
					(alternate "UART_2_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "P1.2")
					(number "9")
					(alternate "GPIO1_2" passive line)
					(alternate "I2C_3_SCL" passive line)
					(alternate "SPI_3_MOSI" passive line)
					(alternate "UART_0_RX" passive line)
					(alternate "UART_3_CTS" passive line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "P1.3")
					(number "10")
					(alternate "GPIO_1_3" passive line)
					(alternate "I2C_3_SDA" passive line)
					(alternate "SPI_3_CLK" passive line)
					(alternate "UART_0_TX" passive line)
					(alternate "UART_3_RTS" passive line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "P1.6")
					(number "11")
					(alternate "GPIO_1_6" passive line)
					(alternate "SPI_1_MISO" passive line)
					(alternate "UART_1_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "P1.4")
					(number "12")
					(alternate "GPIO_1_4" passive line)
					(alternate "SPI_3_MISO" passive line)
					(alternate "SWD_1_CLK" passive line)
					(alternate "UART_3_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "P1.5")
					(number "13")
					(alternate "GPIO_1_5" passive line)
					(alternate "SPI_3_SEL" passive line)
					(alternate "SWD_1_DAT" passive line)
					(alternate "UART_3_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "P1.7")
					(number "14")
					(alternate "GPIO_1_7" passive line)
					(alternate "SPI_1_SEL" passive line)
					(alternate "UART_1_RX" passive line)
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "P2.0")
					(number "15")
					(alternate "GPIO_2_0" passive line)
					(alternate "I2C_1_SCL" passive line)
					(alternate "SPI_1_CLK" passive line)
					(alternate "SWD_0_DAT" passive line)
					(alternate "UART_1_CTS" passive line)
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "P2.1")
					(number "16")
					(alternate "GPIO_2_1" passive line)
					(alternate "I2C_1_SDA" passive line)
					(alternate "SPI_1_MOSI" passive line)
					(alternate "SWD_0_CLK" passive line)
					(alternate "UART_1_RTS" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDD")
					(number "17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDIO")
					(number "18")
				)
				(pin power_out line
					(at 0 -45.72 0)
					(length 2.54)
					(name "VCCD")
					(number "19")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VSYS")
					(number "20")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "DPLUS")
					(number "21")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "DMINUS")
					(number "22")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "P2.4")
					(number "23")
					(alternate "GPIO_2_4" passive line)
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "P2.5")
					(number "24")
					(alternate "GPIO_2_5" passive line)
					(alternate "SPI_0_MOSI" passive line)
					(alternate "UART_0_TX" passive line)
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "P2.6")
					(number "25")
					(alternate "GPIO_2_6" passive line)
					(alternate "SPI_0_CLK" passive line)
					(alternate "UART_0_RX" passive line)
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "XRES")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P0.0")
					(number "27")
					(alternate "GPIO" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P0.1")
					(number "28")
				)
				(pin no_connect line
					(at 13.97 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at 19.05 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin no_connect line
					(at 21.59 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "31")
				)
				(pin no_connect line
					(at 11.43 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "32")
				)
				(pin power_in line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "VSS")
					(number "33")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "P3.2")
					(number "34")
					(alternate "GPIO_3_2" passive line)
					(alternate "TCPWM0" passive line)
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "P3.3")
					(number "35")
					(alternate "GPIO_3_3" passive line)
					(alternate "TCPWM1" passive line)
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "P3.4")
					(number "36")
					(alternate "GPIO_3_4" passive line)
					(alternate "I2C_2_SDA" passive line)
					(alternate "SPI_2_MOSI" passive line)
					(alternate "TCPWM2" passive line)
					(alternate "UART_2_CTS" passive line)
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "P3.5")
					(number "37")
					(alternate "GPIO_3_5" passive line)
					(alternate "I2C_2_SCL" passive line)
					(alternate "SPI_2_CLK" passive line)
					(alternate "TCPWM3" passive line)
					(alternate "UART_2_RTS" passive line)
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "P3.6")
					(number "38")
					(alternate "GPIO_3_6" passive line)
				)
				(pin no_connect line
					(at 13.97 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "39")
				)
				(pin no_connect line
					(at 16.51 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "40")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "EP")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
