(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CYPD3177-24LQXQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CYPD3177-24LQXQ"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CYPD3177-24LQXQ"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD_BCR_Datasheet_USB_Type-C_Port_Controller_for_Power_Sinks-DataSheet-v03_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee7ce9d70ad"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Type-C and Power Delivery (PD) Controller, USB PD 3.0, 2.7 V, 5.5 V, QFN-EP"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CYPD3177-24LQXQ"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, INTERFACE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CYPD3177-24LQXQ_1_1"
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VBUS_MIN")
					(number "1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VBUS_MAX")
					(number "2")
				)
				(pin output line
					(at 33.02 0 180)
					(length 2.54)
					(name "VBUS_FET_EN")
					(number "3")
				)
				(pin output line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "SAFE_PWR_EN")
					(number "4")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "ISNK_COARSE")
					(number "5")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "ISNK_FINE")
					(number "6")
				)
				(pin passive line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "~{HPI_INT}")
					(number "7")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "GPIO_1")
					(number "8")
				)
				(pin output line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "FAULT")
					(number "9")
				)
				(pin open_collector line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "FLIP")
					(number "10")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "VDC_OUT")
					(number "11")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "HPI_SDA")
					(number "12")
				)
				(pin passive line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "HPI_SCL")
					(number "13")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CC2")
					(number "14")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CC1")
					(number "15")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D-")
					(number "16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D+")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBUS_IN")
					(number "18")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin no_connect line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "DNU1")
					(number "20")
				)
				(pin no_connect line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "DNU2")
					(number "21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "22")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "VDDD")
					(number "23")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VCCD")
					(number "24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
