(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CYPD5235-96BZXI"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CYPD5235-96BZXI"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CYPD5235-96BZXI"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD_CCG5_USB_TYPE-C_PORT_CONTROLLER-DataSheet-v14_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee43d546acb&utm_source=cypress&utm_medium=referral&utm_campaign=202110_globe_en_all_integration-files&redirId=File_3_1179"
				(at 71.12 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC Universal USB Type-C and Power Delivery (PD) 3.0 controller 96-NFBGA -40°C to 85"
				(at 71.12 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CYPD5235-96BZXI"
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CYPD5235-96BZXI_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VSYS")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "SWD_IO")
					(number "B2")
					(alternate "P1.6" passive line)
					(alternate "~{AR_RST}" passive line)
				)
				(pin bidirectional line
					(at 52.07 -33.02 180)
					(length 3.81)
					(name "UV_OCP_TRIP_P1")
					(number "B6")
					(alternate "P1.4" passive line)
				)
				(pin bidirectional line
					(at 52.07 -48.26 180)
					(length 3.81)
					(name "UV_OCP_TRIP_P2")
					(number "B7")
					(alternate "P1.5" passive line)
				)
				(pin bidirectional line
					(at 52.07 -30.48 180)
					(length 3.81)
					(name "VCONN_OCP_TRIP_P1")
					(number "B8")
					(alternate "P3.5" passive line)
				)
				(pin bidirectional line
					(at 52.07 -45.72 180)
					(length 3.81)
					(name "VCONN_OCP_TRIP_P2")
					(number "B9")
					(alternate "P3.3" passive line)
				)
				(pin power_out line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VCCD")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "SWD_CLK")
					(number "C2")
					(alternate "I2C_CFG_EC" passive line)
					(alternate "P1.0" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDIO")
					(number "C10")
				)
				(pin bidirectional line
					(at 52.07 -17.78 180)
					(length 3.81)
					(name "I2C_SDA_SCB2_TBT")
					(number "D2")
					(alternate "P1.1" passive line)
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDD")
					(number "D10")
				)
				(pin bidirectional line
					(at 52.07 -15.24 180)
					(length 3.81)
					(name "I2C_SCL_SCB2_TBT")
					(number "E2")
					(alternate "P1.2" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin bidirectional line
					(at 52.07 -10.16 180)
					(length 3.81)
					(name "I2C_INT_TBT_P1")
					(number "F2")
					(alternate "P1.3" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin bidirectional line
					(at 52.07 -22.86 180)
					(length 3.81)
					(name "I2C_SCL_SCB4")
					(number "F10")
					(alternate "P2.3" passive line)
				)
				(pin bidirectional line
					(at 52.07 -12.7 180)
					(length 3.81)
					(name "I2C_INT_TBT_P2")
					(number "G2")
					(alternate "P2.1" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin no_connect line
					(at 3.81 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G8")
				)
				(pin bidirectional line
					(at 52.07 -25.4 180)
					(length 3.81)
					(name "I2C_SDA_SCB4")
					(number "G10")
					(alternate "P3.2" passive line)
				)
				(pin no_connect line
					(at 3.81 -45.72 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H4")
				)
				(pin no_connect line
					(at 3.81 -48.26 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H5")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "XRES")
					(number "H6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin no_connect line
					(at 3.81 -50.8 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H8")
				)
				(pin bidirectional line
					(at 52.07 -55.88 180)
					(length 3.81)
					(name "VSEL_2_P2")
					(number "H10")
					(alternate "P2.0" passive line)
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "V5V_P1")
					(number "J2")
				)
				(pin bidirectional line
					(at 52.07 -40.64 180)
					(length 3.81)
					(name "VSEL_2_P1")
					(number "J10")
					(alternate "P3.6" passive line)
					(alternate "VSEL_2_P1" passive line)
				)
				(pin bidirectional line
					(at 52.07 -35.56 180)
					(length 3.81)
					(name "OVP_TRIP_P1")
					(number "K5")
					(alternate "OVP_TRIP_P1" passive line)
					(alternate "P2.4" passive line)
				)
				(pin bidirectional line
					(at 52.07 -5.08 180)
					(length 3.81)
					(name "I2C_SDA_SCB1_EC")
					(number "K6")
					(alternate "P5.0" passive line)
				)
				(pin bidirectional line
					(at 52.07 -53.34 180)
					(length 3.81)
					(name "VSEL_1_P2")
					(number "L4")
					(alternate "P0.0" passive line)
				)
				(pin bidirectional line
					(at 52.07 0 180)
					(length 3.81)
					(name "I2C_INT_EC")
					(number "L5")
					(alternate "P2.5" passive line)
				)
				(pin bidirectional line
					(at 52.07 -2.54 180)
					(length 3.81)
					(name "I2C_SCL_SCB1_EC")
					(number "L6")
					(alternate "P5.1" passive line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "P3.1")
					(number "L7")
				)
				(pin bidirectional line
					(at 52.07 -50.8 180)
					(length 3.81)
					(name "OVP_TRIP_P2")
					(number "L8")
					(alternate "P2.2" passive line)
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "V5V_P2")
					(number "L9")
				)
				(pin bidirectional line
					(at 52.07 -38.1 180)
					(length 3.81)
					(name "VSEL_1_P1")
					(number "L10")
					(alternate "P3.7" passive line)
					(alternate "VSEL_1_P1" passive line)
				)
			)
			(symbol "CYPD5235-96BZXI_2_1"
				(pin bidirectional line
					(at 52.07 -15.24 180)
					(length 3.81)
					(name "DPLUS_TOP_P1")
					(number "A1")
				)
				(pin bidirectional line
					(at 52.07 -17.78 180)
					(length 3.81)
					(name "DMINUS_TOP_P1")
					(number "A2")
				)
				(pin bidirectional line
					(at 52.07 -7.62 180)
					(length 3.81)
					(name "SBU1_P1")
					(number "A3")
				)
				(pin bidirectional line
					(at 52.07 -10.16 180)
					(length 3.81)
					(name "SBU2_P1")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DPLUS_SYS_P1")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DMINUS_SYS_P1")
					(number "A7")
				)
				(pin bidirectional line
					(at 52.07 -40.64 180)
					(length 3.81)
					(name "UART_TX_P1")
					(number "A8")
					(alternate "P4.0" passive line)
				)
				(pin bidirectional line
					(at 52.07 -43.18 180)
					(length 3.81)
					(name "UART_RX_P1")
					(number "A9")
					(alternate "P4.1" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "LSTX_P1")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "LSRX_P1")
					(number "A11")
				)
				(pin bidirectional line
					(at 52.07 -22.86 180)
					(length 3.81)
					(name "DPLUS_BOT_P1")
					(number "B1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CSN_P1")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "AUX_P_P1")
					(number "B11")
				)
				(pin bidirectional line
					(at 52.07 -25.4 180)
					(length 3.81)
					(name "DMINUS_BOT_P1")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "AUX_N_P1")
					(number "C11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VBUS_P1")
					(number "D1")
				)
				(pin passive line
					(at 52.07 -2.54 180)
					(length 3.81)
					(name "CC2_P1")
					(number "H2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "CSP_P1")
					(number "J1")
				)
				(pin passive line
					(at 52.07 0 180)
					(length 3.81)
					(name "CC1_P1")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VBUS_P_CTRL_P1")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VBUS_C_CTRL_P1")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "HPD_P1")
					(number "K7")
					(alternate "P3.0" passive line)
				)
			)
			(symbol "CYPD5235-96BZXI_3_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VBUS_P_CTRL_P2")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VBUS_C_CTRL_P2")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "AUX_P_P2")
					(number "D11")
				)
				(pin bidirectional line
					(at 52.07 -7.62 180)
					(length 3.81)
					(name "SBU1_P2")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "HPD_P2")
					(number "E10")
					(alternate "P3.4" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "AUX_N_P2")
					(number "E11")
				)
				(pin bidirectional line
					(at 52.07 -10.16 180)
					(length 3.81)
					(name "SBU2_P2")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DPLUS_SYS_P2")
					(number "F11")
				)
				(pin bidirectional line
					(at 52.07 -15.24 180)
					(length 3.81)
					(name "DPLUS_TOP_P2")
					(number "G1")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DMINUS_SYS_P2")
					(number "G11")
				)
				(pin bidirectional line
					(at 52.07 -17.78 180)
					(length 3.81)
					(name "DMINUS_TOP_P2")
					(number "H1")
				)
				(pin bidirectional line
					(at 52.07 -40.64 180)
					(length 3.81)
					(name "UART_TX_P2")
					(number "H11")
					(alternate "P0.1" passive line)
				)
				(pin bidirectional line
					(at 52.07 -43.18 180)
					(length 3.81)
					(name "UART_RX_P2")
					(number "J11")
					(alternate "P0.2" passive line)
				)
				(pin bidirectional line
					(at 52.07 -22.86 180)
					(length 3.81)
					(name "DPLUS_BOT_P2")
					(number "K1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CSN_P2")
					(number "K8")
				)
				(pin passive line
					(at 52.07 0 180)
					(length 3.81)
					(name "CC1_P2")
					(number "K9")
				)
				(pin passive line
					(at 52.07 -2.54 180)
					(length 3.81)
					(name "CC2_P2")
					(number "K10")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "LSTX_P2")
					(number "K11")
				)
				(pin bidirectional line
					(at 52.07 -25.4 180)
					(length 3.81)
					(name "DMINUS_BOT_P2")
					(number "L1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "CSP_P2")
					(number "L2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VBUS_P2")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "LSRX_P2")
					(number "L11")
				)
			)
			(embedded_fonts no)
		)
)
