(footprint "USB-C_Receptacle_JAE_DX07S024JJ2"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.726 -5.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-C_Receptacle_JAE_DX07S024JJ2"
		(at -5 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "PCB EDGE"
		(at 5.5 3.1 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Author: Antmicro"
		(at -5.571 7.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.571 8.8 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.571 10 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.601 -1.115)
		(size 0.63 0.63)
		(drill 0.63)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole oval
		(at 3.6 -1.18)
		(size 0.88 0.53)
		(drill oval 0.88 0.53)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd rect
		(at -2.625 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.125 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -1.625 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -1.125 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -0.625 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.125 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.374 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 0.874 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 1.374 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 1.874 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 2.374 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 2.874 -3.817)
		(size 0.27 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at 2.624 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd rect
		(at 2.124 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd rect
		(at 1.624 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at 1.124 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd rect
		(at 0.624 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd rect
		(at 0.124 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd rect
		(at -0.375 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd rect
		(at -0.875 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd rect
		(at -1.375 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd rect
		(at -1.875 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd rect
		(at -2.375 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd rect
		(at -2.875 -2.215)
		(size 0.27 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -4.321 1.933)
		(size 1.3 2.6)
		(drill oval 0.75 2.05)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole custom
		(at -4.32 -3.12)
		(size 1.2 1.2)
		(drill oval 0.6 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_line
				(start 0.6 0.6)
				(end 0 0.6)
				(width 1.1)
			)
			(gr_line
				(start 0 -0.55)
				(end 0 0.55)
				(width 1.2)
			)
		)
	)
	(pad "SH" thru_hole oval
		(at -3.99 -2.52 90)
		(size 1 1.55)
		(drill oval 0.7 1.25)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.99 -2.52 270)
		(size 1 1.55)
		(drill oval 0.7 1.25)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole custom
		(at 4.32 -3.12)
		(size 1.2 1.2)
		(drill oval 0.6 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_line
				(start -0.6 0.6)
				(end 0 0.6)
				(width 1.1)
			)
			(gr_line
				(start 0 -0.55)
				(end 0 0.55)
				(width 1.2)
			)
		)
	)
	(pad "SH" thru_hole oval
		(at 4.32 1.933)
		(size 1.3 2.6)
		(drill oval 0.75 2.05)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(layer "F.Cu")
		(name "TOP_KEEPOUT")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 3.899008 -0.830008) (xy 3.099736 -0.829927) (xy 3.098728 -1.515919) (xy -3.24 -1.516) (xy -3.24 -0.75)
				(xy -3.9 -0.75) (xy -3.9 0.633) (xy -3.551 0.633) (xy -3.551 3.233) (xy -3.9 3.233) (xy -3.9 3.733)
				(xy 3.899 3.733) (xy 3.899 3.233) (xy 3.55 3.233) (xy 3.55 0.633) (xy 3.899 0.633)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_dx07s024jj2.glb"
		(offset
			(xyz 0 0.5 1.6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "antmicro_dx07s024jj2.glb"
		(offset
			(xyz 0 -4.5 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -0 -0)
		)
	)
)
