(footprint "USB-C_Plug_JAE_DX07VN24WA2C1568_Vertical"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "USB-C_Plug_JAE_DX07VN24WA2C1568_Vertical"
		(at 0 6.499 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -9.2 8.499 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.2 9.699 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.2 10.899 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -7.701 0 180)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.701 1.999 180)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.7 0)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.7 1.999)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd rect
		(at 2.749 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at 2.249 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at 1.749 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at 1.249 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at 0.749 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at 0.249 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at -0.25 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at -0.75 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at -1.25 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at -1.75 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at -2.25 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at -2.75 -2.3)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at -2.75 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd rect
		(at -2.25 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd rect
		(at -1.75 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at -1.25 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd rect
		(at -0.75 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd rect
		(at -0.25 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd rect
		(at 0.249 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd rect
		(at 0.749 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd rect
		(at 1.249 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd rect
		(at 1.749 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd rect
		(at 2.249 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd rect
		(at 2.749 2.299 180)
		(size 0.27 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -4.05 -2.3 180)
		(size 1.75 0.95)
		(drill oval 1.35 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.05 0 180)
		(size 1.5 1)
		(drill oval 1.1 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.05 2.299 180)
		(size 1.75 0.95)
		(drill oval 1.35 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.049 -2.3)
		(size 1.75 0.95)
		(drill oval 1.35 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.049 0)
		(size 1.5 1)
		(drill oval 1.1 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.049 2.299)
		(size 1.75 0.95)
		(drill oval 1.35 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_dx07vn24wa2c1568.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
