(footprint "USB-C_Receptacle_PulseElectronics_E8124-015-01"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.digikey.com/product-detail/en/pulse-electronics-network/E8124-015-01/553-3195-2-ND/5800435")
	(property "Reference" "REF**"
		(at 0 -2.64 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-C_Receptacle_PulseElectronics_E8124-015-01"
		(at 0 9.29 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.2 11.29 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.2 12.49 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.2 13.69 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.6 0.57)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd rect
		(at -1.25 -0.98)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.25 -0.98)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" np_thru_hole oval
		(at 3.6 0.57)
		(size 0.95 0.65)
		(drill oval 0.95 0.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd rect
		(at -2.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -1.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -1.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -0.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 0.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 1.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 1.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 2.25 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 2.75 0)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" thru_hole circle
		(at 2.8 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B2" thru_hole circle
		(at 2.4 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B3" thru_hole circle
		(at 1.6 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at 1.2 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at 0.8 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at 0.4 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at -0.4 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at -0.8 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at -1.2 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B10" thru_hole circle
		(at -1.6 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B11" thru_hole circle
		(at -2.4 1.92)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at -2.8 1.22)
		(size 0.65 0.65)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.5 4.335)
		(size 0.9 1.9)
		(drill oval 0.5 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -4.22 1.82)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -3.845 -0.98)
		(size 1.15 0.9)
		(drill oval 0.75 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.845 -0.98)
		(size 1.15 0.9)
		(drill oval 0.75 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.22 1.82)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 4.5 4.335)
		(size 0.9 1.9)
		(drill oval 0.5 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_e8124_015_01.glb"
		(offset
			(xyz 0 -4.8 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "antmicro_e8124_015_01.glb"
		(offset
			(xyz 0 -8.3 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
