(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "F52R-1A7H1-11020"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "F52R-1A7H1-11020"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "F52R-1A7H1-11020"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/f52r.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FFC / FPC Board Connector, R/A, ZIF, 1 mm, 20 Contacts, Receptacle, F52R, Surface Mount, Bottom"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "F52R-1A7H1-11020"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "F52R-1A7H1-11020_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "9")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "10")
					(number "10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "11")
					(number "11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "12")
					(number "12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "13")
					(number "13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "14")
					(number "14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "15")
					(number "15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "16")
					(number "16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "17")
					(number "17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "18")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "19")
					(number "19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "20")
					(number "20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "MP1")
					(number "MP1")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "MP2")
					(number "MP2")
				)
			)
			(embedded_fonts no)
		)
)
