(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT2232D"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -4.064 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT2232D"
				(at 48.26 -9.144 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT2232D"
				(at 48.26 -11.684 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2020/08/DS_FT2232D.pdf"
				(at 48.26 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface Bridges, USB to UART, FIFO, 3 V, 5.25 V, LQFP, 48 Pins, -40 °C"
				(at 48.26 -26.924 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT2232D"
				(at 48.26 -6.604 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 48.26 -16.764 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -21.844 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -24.384 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT2232D_1_1"
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EESCK")
					(number "1")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "EEDATA")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RESET#")
					(number "4")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RSTOUT#")
					(number "5")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "3V3OUT")
					(number "6")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "USBDP")
					(number "7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "USBDM")
					(number "8")
				)
				(pin passive line
					(at 0 -71.374 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin passive line
					(at 33.02 -34.29 180)
					(length 2.54)
					(name "SI/WUA")
					(number "10")
				)
				(pin passive line
					(at 33.02 -31.75 180)
					(length 2.54)
					(name "ACBUS3")
					(number "11")
				)
				(pin passive line
					(at 33.02 -29.21 180)
					(length 2.54)
					(name "ACBUS2")
					(number "12")
				)
				(pin passive line
					(at 33.02 -26.67 180)
					(length 2.54)
					(name "ACBUS1")
					(number "13")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCCIOA")
					(number "14")
				)
				(pin passive line
					(at 33.02 -24.13 180)
					(length 2.54)
					(name "ACBUS0")
					(number "15")
				)
				(pin passive line
					(at 33.02 -19.05 180)
					(length 2.54)
					(name "ADBUS7")
					(number "16")
				)
				(pin passive line
					(at 33.02 -16.51 180)
					(length 2.54)
					(name "ADBUS6")
					(number "17")
				)
				(pin passive line
					(at 0 -71.374 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin passive line
					(at 33.02 -13.97 180)
					(length 2.54)
					(name "ADBUS5")
					(number "19")
				)
				(pin passive line
					(at 33.02 -11.43 180)
					(length 2.54)
					(name "ADBUS4")
					(number "20")
				)
				(pin passive line
					(at 33.02 -8.89 180)
					(length 2.54)
					(name "ADBUS3")
					(number "21")
				)
				(pin passive line
					(at 33.02 -6.35 180)
					(length 2.54)
					(name "ADBUS2")
					(number "22")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "ADBUS1")
					(number "23")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 2.54)
					(name "ADBUS0")
					(number "24")
				)
				(pin passive line
					(at 0 -71.374 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin passive line
					(at 33.02 -72.644 180)
					(length 2.54)
					(name "SI/WUB")
					(number "26")
				)
				(pin passive line
					(at 33.02 -69.85 180)
					(length 2.54)
					(name "BCBUS3")
					(number "27")
				)
				(pin passive line
					(at 33.02 -67.31 180)
					(length 2.54)
					(name "BCBUS2")
					(number "28")
				)
				(pin passive line
					(at 33.02 -64.77 180)
					(length 2.54)
					(name "BCBUS1")
					(number "29")
				)
				(pin passive line
					(at 33.02 -62.23 180)
					(length 2.54)
					(name "BCBUS0")
					(number "30")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCCIOB")
					(number "31")
				)
				(pin passive line
					(at 33.02 -57.15 180)
					(length 2.54)
					(name "BDBUS7")
					(number "32")
				)
				(pin passive line
					(at 33.02 -54.61 180)
					(length 2.54)
					(name "BDBUS6")
					(number "33")
				)
				(pin passive line
					(at 0 -71.374 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
				(pin passive line
					(at 33.02 -52.07 180)
					(length 2.54)
					(name "BDBUS5")
					(number "35")
				)
				(pin passive line
					(at 33.02 -49.53 180)
					(length 2.54)
					(name "BDBUS4")
					(number "36")
				)
				(pin passive line
					(at 33.02 -46.99 180)
					(length 2.54)
					(name "BDBUS3")
					(number "37")
				)
				(pin passive line
					(at 33.02 -44.45 180)
					(length 2.54)
					(name "BDBUS2")
					(number "38")
				)
				(pin passive line
					(at 33.02 -41.91 180)
					(length 2.54)
					(name "BDBUS1")
					(number "39")
				)
				(pin passive line
					(at 33.02 -39.37 180)
					(length 2.54)
					(name "BDBUS0")
					(number "40")
				)
				(pin passive line
					(at 33.02 -76.454 180)
					(length 2.54)
					(name "PWREN#")
					(number "41")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "42")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "XTIN")
					(number "43")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "XTOUT")
					(number "44")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "AGND")
					(number "45")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "AVCC")
					(number "46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "TEST")
					(number "47")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "EECS")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
