(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT2232HL-REEL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT2232HL-REEL"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT2232HL-REEL"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1700960.pdf"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface Bridges, USB to UART, FIFO, 1.62 V, 3.63 V, LQFP, 64 Pins, -40 °C"
				(at 48.26 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT2232HL-REEL"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, I2C, USB, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT2232HL-REEL_1_1"
				(pin power_in line
					(at 0 -83.82 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "OSCI")
					(number "2")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 2.54)
					(name "OSCO")
					(number "3")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VPHY")
					(number "4")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "REF")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "DM")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DP")
					(number "8")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "VPLL")
					(number "9")
				)
				(pin power_in line
					(at 0 -86.36 0)
					(length 2.54)
					(name "AGND")
					(number "10")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "VCORE")
					(number "12")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 2.54)
					(name "TEST")
					(number "13")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "~{RESET}")
					(number "14")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin bidirectional line
					(at 33.02 0 180)
					(length 2.54)
					(name "ADBUS0")
					(number "16")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "ADBUS1")
					(number "17")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "ADBUS2")
					(number "18")
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "ADBUS3")
					(number "19")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VCCIO")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 2.54)
					(name "ADBUS4")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "ADBUS5")
					(number "22")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "ADBUS6")
					(number "23")
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "ADBUS7")
					(number "24")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "ACBUS0")
					(number "26")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "ACBUS1")
					(number "27")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "ACBUS2")
					(number "28")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "ACBUS3")
					(number "29")
				)
				(pin bidirectional line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "ACBUS4")
					(number "30")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "31")
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 2.54)
					(name "ACBUS5")
					(number "32")
				)
				(pin bidirectional line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "ACBUS6")
					(number "33")
				)
				(pin bidirectional line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "ACBUS7")
					(number "34")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "35")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 2.54)
					(name "~{SUSPEND}")
					(number "36")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "VCORE")
					(number "37")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 2.54)
					(name "BDBUS0")
					(number "38")
				)
				(pin bidirectional line
					(at 33.02 -71.12 180)
					(length 2.54)
					(name "BDBUS1")
					(number "39")
				)
				(pin bidirectional line
					(at 33.02 -73.66 180)
					(length 2.54)
					(name "BDBUS2")
					(number "40")
				)
				(pin bidirectional line
					(at 33.02 -76.2 180)
					(length 2.54)
					(name "BDBUS3")
					(number "41")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "42")
				)
				(pin bidirectional line
					(at 33.02 -78.74 180)
					(length 2.54)
					(name "BDBUS4")
					(number "43")
				)
				(pin bidirectional line
					(at 33.02 -81.28 180)
					(length 2.54)
					(name "BDBUS5")
					(number "44")
				)
				(pin bidirectional line
					(at 33.02 -83.82 180)
					(length 2.54)
					(name "BDBUS6")
					(number "45")
				)
				(pin bidirectional line
					(at 33.02 -86.36 180)
					(length 2.54)
					(name "BDBUS7")
					(number "46")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "BCBUS0")
					(number "48")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VREGOUT")
					(number "49")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VREGIN")
					(number "50")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 2.54)
					(name "BCBUS1")
					(number "52")
				)
				(pin bidirectional line
					(at 33.02 -50.8 180)
					(length 2.54)
					(name "BCBUS2")
					(number "53")
				)
				(pin bidirectional line
					(at 33.02 -53.34 180)
					(length 2.54)
					(name "BCBUS3")
					(number "54")
				)
				(pin bidirectional line
					(at 33.02 -55.88 180)
					(length 2.54)
					(name "BCBUS4")
					(number "55")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "56")
				)
				(pin bidirectional line
					(at 33.02 -58.42 180)
					(length 2.54)
					(name "BCBUS5")
					(number "57")
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 2.54)
					(name "BCBUS6")
					(number "58")
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 2.54)
					(name "BCBUS7")
					(number "59")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 2.54)
					(name "~{PWREN}")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "EEDATA")
					(number "61")
				)
				(pin output clock
					(at 0 -60.96 0)
					(length 2.54)
					(name "EECLK")
					(number "62")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "EECS")
					(number "63")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "VCORE")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
