(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT231XQ-R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT231XQ-R"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT231XQ-R"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2021/10/DS_FT231X.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB-UART Converter, USB 2.0, 2.97 V, 5.5 V, SSOP, 20 Pins"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT231XQ-R"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, USB, UART, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT231XQ-R_1_1"
				(pin input line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "RXD")
					(number "1")
				)
				(pin input line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "~{RI}")
					(number "2")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "~{DSR}")
					(number "4")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "~{DCD}")
					(number "5")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "~{CTS}")
					(number "6")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "CBUS2")
					(number "7")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "USBDP")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "USBDM")
					(number "9")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 2.54)
					(name "3V3OUT")
					(number "10")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{RESET}")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "12")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "CBUS1")
					(number "14")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "CBUS0")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "CBUS3")
					(number "16")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "TXD")
					(number "17")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "~{DTR}")
					(number "18")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "~{RTS}")
					(number "19")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCCIO")
					(number "20")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
