(footprint "DFN-12-1EP_3x3mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "http://www.ftdichip.com/Support/Documents/TechnicalNotes/TN_166%20FTDI%20Example%20IC%20PCB%20Footprints.pdf")
	(property "Reference" "REF**"
		(at 0 -2.926 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-12-1EP_3x3mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.101 3.6 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.101 4.799 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.101 5.999 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.551 -1.125 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.551 -0.677 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.551 -0.227 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.551 0.225 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.551 0.675 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.551 1.124 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.55 1.124 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.55 0.675 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.55 0.225 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.55 -0.227 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.55 -0.677 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.55 -1.125 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0 0 270)
		(size 2.5 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_ft234xd_r.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
