(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT4222HQ-D-R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 59.69 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT4222HQ-D-R"
				(at 59.69 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT4222HQ-D-R"
				(at 59.69 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4222H.pdf"
				(at 59.69 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC USB 2.0 to Quad SPI I2C Bridge 53.8Mbps"
				(at 59.69 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 59.69 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT4222HQ-D-R"
				(at 59.69 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 59.69 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 59.69 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, USB, SPI, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT4222HQ-D-R_1_1"
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DEBUGGER")
					(number "1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "STEST_RSTN")
					(number "2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "~{RESET}")
					(number "3")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DCNF0")
					(number "4")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DCNF1")
					(number "5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCIO")
					(number "7")
				)
				(pin bidirectional line
					(at 46.99 0 180)
					(length 5.08)
					(name "SCK")
					(number "8")
				)
				(pin bidirectional line
					(at 46.99 -5.08 180)
					(length 5.08)
					(name "MISO")
					(number "9")
				)
				(pin bidirectional line
					(at 46.99 -2.54 180)
					(length 5.08)
					(name "MOSI")
					(number "10")
				)
				(pin bidirectional line
					(at 46.99 -7.62 180)
					(length 5.08)
					(name "IO2")
					(number "11")
				)
				(pin bidirectional line
					(at 46.99 -10.16 180)
					(length 5.08)
					(name "IO3")
					(number "12")
				)
				(pin bidirectional line
					(at 46.99 -20.32 180)
					(length 5.08)
					(name "GPIO0/SS1O/SCL")
					(number "13")
				)
				(pin bidirectional line
					(at 46.99 -22.86 180)
					(length 5.08)
					(name "GPIO1/SS2O/SDA")
					(number "14")
				)
				(pin bidirectional line
					(at 46.99 -25.4 180)
					(length 5.08)
					(name "GPIO2/SS3O/SUSP_OUT")
					(number "15")
				)
				(pin bidirectional line
					(at 46.99 -27.94 180)
					(length 5.08)
					(name "GPIO3/WAKEUP/INTR")
					(number "16")
				)
				(pin output line
					(at 46.99 -17.78 180)
					(length 5.08)
					(name "SS0O")
					(number "17")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "XSCI")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "XSCO")
					(number "19")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "RREF")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DM")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "DP")
					(number "23")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VOUT3V3")
					(number "25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCCIN")
					(number "26")
				)
				(pin power_in line
					(at 46.99 -38.1 180)
					(length 5.08)
					(name "AGND")
					(number "27")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VPP")
					(number "29")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VBUS_DET")
					(number "30")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "BCD_DET")
					(number "31")
				)
				(pin input line
					(at 46.99 -12.7 180)
					(length 5.08)
					(name "SS")
					(number "32")
				)
				(pin passive line
					(at 46.99 -35.56 180)
					(length 5.08)
					(name "EP")
					(number "33")
				)
				(pin power_in line
					(at 46.99 -43.18 180)
					(length 5.08)
					(name "DGND")
					(number "[6,28]")
				)
				(pin power_in line
					(at 46.99 -48.26 180)
					(length 5.08)
					(name "UGND")
					(number "[20,24]")
				)
			)
			(embedded_fonts no)
		)
)
