(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT4232HP_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT4232HP_QFN"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT4232HP_QFN"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2021/11/DS_FT4233HP.pdf"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface Bridges, USB to UART, MPSSE, 1.62 V, 1.98 V, LQFP, 64 Pins, -40 °C"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT4232HPQ-TRAY"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, USB, UART, I2C, SPI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT4232HP_QFN_1_1"
				(pin output line
					(at 0 -53.34 0)
					(length 2.54)
					(name "EECLK")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "EEDATA")
					(number "2")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 2.54)
					(name "TEST")
					(number "3")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "~{RESET}")
					(number "4")
				)
				(pin bidirectional line
					(at 40.64 -93.98 180)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 2.54)
					(name "ADBUS0")
					(number "6")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 2.54)
					(name "ADBUS1")
					(number "7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "V_{CORE}")
					(number "8")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{CCIO}")
					(number "10")
				)
				(pin bidirectional line
					(at 40.64 -5.08 180)
					(length 2.54)
					(name "ADBUS2")
					(number "11")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 2.54)
					(name "ADBUS3")
					(number "12")
				)
				(pin bidirectional line
					(at 40.64 -10.16 180)
					(length 2.54)
					(name "ADBUS4")
					(number "13")
				)
				(pin bidirectional line
					(at 40.64 -12.7 180)
					(length 2.54)
					(name "ADBUS5")
					(number "14")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 2.54)
					(name "ADBUS6")
					(number "15")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 2.54)
					(name "ADBUS7")
					(number "16")
				)
				(pin bidirectional line
					(at 40.64 -21.59 180)
					(length 2.54)
					(name "BDBUS0")
					(number "17")
				)
				(pin bidirectional line
					(at 40.64 -24.13 180)
					(length 2.54)
					(name "BDBUS1")
					(number "18")
				)
				(pin bidirectional line
					(at 40.64 -26.67 180)
					(length 2.54)
					(name "BDBUS2")
					(number "19")
				)
				(pin bidirectional line
					(at 40.64 -29.21 180)
					(length 2.54)
					(name "BDBUS3")
					(number "20")
				)
				(pin bidirectional line
					(at 40.64 -31.75 180)
					(length 2.54)
					(name "BDBUS4")
					(number "21")
				)
				(pin bidirectional line
					(at 40.64 -34.29 180)
					(length 2.54)
					(name "BDBUS5")
					(number "22")
				)
				(pin bidirectional line
					(at 40.64 -36.83 180)
					(length 2.54)
					(name "BDBUS6")
					(number "23")
				)
				(pin bidirectional line
					(at 40.64 -39.37 180)
					(length 2.54)
					(name "BDBUS7")
					(number "24")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "V_{CORE}")
					(number "25")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "V_{CCIO}")
					(number "26")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 2.54)
					(name "OSCI")
					(number "27")
				)
				(pin output line
					(at 0 -67.31 0)
					(length 2.54)
					(name "OSCO")
					(number "28")
				)
				(pin power_in line
					(at 0 -101.6 0)
					(length 2.54)
					(name "GND")
					(number "29")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{REGIN}")
					(number "30")
				)
				(pin power_out line
					(at 0 -11.43 0)
					(length 2.54)
					(name "V_{REGOUT}")
					(number "31")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "F_{SOURCE}")
					(number "32")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 2.54)
					(name "V_{PP}")
					(number "33")
				)
				(pin bidirectional line
					(at 40.64 -43.18 180)
					(length 2.54)
					(name "CDBUS0")
					(number "34")
				)
				(pin bidirectional line
					(at 40.64 -45.72 180)
					(length 2.54)
					(name "CDBUS1")
					(number "35")
				)
				(pin bidirectional line
					(at 40.64 -48.26 180)
					(length 2.54)
					(name "CDBUS2")
					(number "36")
				)
				(pin bidirectional line
					(at 40.64 -50.8 180)
					(length 2.54)
					(name "CDBUS3")
					(number "37")
				)
				(pin bidirectional line
					(at 40.64 -53.34 180)
					(length 2.54)
					(name "CDBUS4")
					(number "38")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "V_{CCIO}")
					(number "39")
				)
				(pin bidirectional line
					(at 40.64 -55.88 180)
					(length 2.54)
					(name "CDBUS5")
					(number "40")
				)
				(pin bidirectional line
					(at 40.64 -58.42 180)
					(length 2.54)
					(name "CDBUS6")
					(number "41")
				)
				(pin bidirectional line
					(at 40.64 -60.96 180)
					(length 2.54)
					(name "CDBUS7")
					(number "42")
				)
				(pin output line
					(at 40.64 -100.33 180)
					(length 2.54)
					(name "~{SUSPEND}")
					(number "43")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "V_{CORE}")
					(number "44")
				)
				(pin bidirectional line
					(at 40.64 -64.77 180)
					(length 2.54)
					(name "DDBUS0")
					(number "45")
				)
				(pin bidirectional line
					(at 40.64 -67.31 180)
					(length 2.54)
					(name "DDBUS1")
					(number "46")
				)
				(pin bidirectional line
					(at 40.64 -69.85 180)
					(length 2.54)
					(name "DDBUS2")
					(number "47")
				)
				(pin bidirectional line
					(at 40.64 -72.39 180)
					(length 2.54)
					(name "DDBUS3")
					(number "48")
				)
				(pin bidirectional line
					(at 40.64 -74.93 180)
					(length 2.54)
					(name "DDBUS4")
					(number "49")
				)
				(pin bidirectional line
					(at 40.64 -77.47 180)
					(length 2.54)
					(name "DDBUS5")
					(number "50")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "V_{CCIO}")
					(number "51")
				)
				(pin bidirectional line
					(at 40.64 -82.55 180)
					(length 2.54)
					(name "DDBUS6")
					(number "52")
				)
				(pin bidirectional line
					(at 40.64 -80.01 180)
					(length 2.54)
					(name "DDBUS7")
					(number "53")
				)
				(pin bidirectional line
					(at 40.64 -91.44 180)
					(length 2.54)
					(name "GPIO2")
					(number "54")
				)
				(pin bidirectional line
					(at 40.64 -88.9 180)
					(length 2.54)
					(name "GPIO1")
					(number "55")
				)
				(pin bidirectional line
					(at 40.64 -86.36 180)
					(length 2.54)
					(name "GPIO0")
					(number "56")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V_{CC_USB}")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "D-")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "D+")
					(number "59")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 2.54)
					(name "REF")
					(number "60")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "V_{CC_PD}")
					(number "61")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PD1_{CC2}")
					(number "62")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PD1_{SVBUS}")
					(number "63")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PD1_{VCONN}")
					(number "64")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PD1_{CC1}")
					(number "65")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "V_{CORE}")
					(number "66")
				)
				(pin output line
					(at 40.64 -97.79 180)
					(length 2.54)
					(name "~{PWREN}")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EECS")
					(number "68")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 2.54)
					(name "EP")
					(number "69")
				)
			)
			(embedded_fonts no)
		)
)
