(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FT4233HPQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FT4233HPQ"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FT4233HPQ"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2023/09/DS_FT4233HP-v1.5.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Hi-Speed/Quad Channel Serial UART/JTAG/SPI/I2C,Dual PD Ports IC"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FT4233HPQ-REEL"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "FTDI Chip"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, USB, UART, I2C, SPI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FT4233HPQ_1_1"
				(pin output clock
					(at 0 -45.72 0)
					(length 2.54)
					(name "EECLK")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "EEDATA")
					(number "2")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 2.54)
					(name "TEST")
					(number "3")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "~{RESET}")
					(number "4")
				)
				(pin bidirectional line
					(at 31.75 -93.98 180)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at 31.75 -96.52 180)
					(length 2.54)
					(name "GPIO4")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -99.06 180)
					(length 2.54)
					(name "GPIO5")
					(number "7")
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 2.54)
					(name "ADBUS0")
					(number "8")
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "ADBUS1")
					(number "9")
				)
				(pin power_in line
					(at 0 -96.52 0)
					(length 2.54)
					(name "VCORE")
					(number "10")
				)
				(pin power_in line
					(at 0 -104.14 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCCIO")
					(number "12")
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 2.54)
					(name "ADBUS2")
					(number "13")
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "ADBUS3")
					(number "14")
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "ADBUS4")
					(number "15")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "ADBUS5")
					(number "16")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "ADBUS6")
					(number "17")
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 2.54)
					(name "ADBUS7")
					(number "18")
				)
				(pin bidirectional line
					(at 31.75 -21.59 180)
					(length 2.54)
					(name "BDBUS0")
					(number "19")
				)
				(pin bidirectional line
					(at 31.75 -24.13 180)
					(length 2.54)
					(name "BDBUS1")
					(number "20")
				)
				(pin bidirectional line
					(at 31.75 -26.67 180)
					(length 2.54)
					(name "BDBUS2")
					(number "21")
				)
				(pin bidirectional line
					(at 31.75 -29.21 180)
					(length 2.54)
					(name "BDBUS3")
					(number "22")
				)
				(pin bidirectional line
					(at 31.75 -31.75 180)
					(length 2.54)
					(name "BDBUS4")
					(number "23")
				)
				(pin bidirectional line
					(at 31.75 -34.29 180)
					(length 2.54)
					(name "BDBUS5")
					(number "24")
				)
				(pin bidirectional line
					(at 31.75 -36.83 180)
					(length 2.54)
					(name "BDBUS6")
					(number "25")
				)
				(pin bidirectional line
					(at 31.75 -39.37 180)
					(length 2.54)
					(name "BDBUS7")
					(number "26")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 2.54)
					(hide yes)
					(name "VCORE")
					(number "27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "28")
				)
				(pin input line
					(at 0 -77.47 0)
					(length 2.54)
					(name "OSCI")
					(number "29")
				)
				(pin output line
					(at 0 -82.55 0)
					(length 2.54)
					(name "OSCO")
					(number "30")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VREGIN")
					(number "32")
				)
				(pin output line
					(at 0 -93.98 0)
					(length 2.54)
					(name "VREGOUT")
					(number "33")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "FSOURCE")
					(number "34")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "VPP")
					(number "35")
				)
				(pin bidirectional line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "CDBUS0")
					(number "36")
				)
				(pin bidirectional line
					(at 31.75 -45.72 180)
					(length 2.54)
					(name "CDBUS1")
					(number "37")
				)
				(pin bidirectional line
					(at 31.75 -48.26 180)
					(length 2.54)
					(name "CDBUS2")
					(number "38")
				)
				(pin bidirectional line
					(at 31.75 -50.8 180)
					(length 2.54)
					(name "CDBUS3")
					(number "39")
				)
				(pin bidirectional line
					(at 31.75 -53.34 180)
					(length 2.54)
					(name "CDBUS4")
					(number "40")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "41")
				)
				(pin bidirectional line
					(at 31.75 -55.88 180)
					(length 2.54)
					(name "CDBUS5")
					(number "42")
				)
				(pin bidirectional line
					(at 31.75 -58.42 180)
					(length 2.54)
					(name "CDBUS6")
					(number "43")
				)
				(pin bidirectional line
					(at 31.75 -60.96 180)
					(length 2.54)
					(name "CDBUS7")
					(number "44")
				)
				(pin output line
					(at 0 -73.66 0)
					(length 2.54)
					(name "~{SUSPEND}")
					(number "45")
				)
				(pin bidirectional line
					(at 31.75 -101.6 180)
					(length 2.54)
					(name "GPIO6")
					(number "46")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 2.54)
					(hide yes)
					(name "VCORE")
					(number "47")
				)
				(pin bidirectional line
					(at 31.75 -64.77 180)
					(length 2.54)
					(name "DDBUS0")
					(number "48")
				)
				(pin bidirectional line
					(at 31.75 -67.31 180)
					(length 2.54)
					(name "DDBUS1")
					(number "49")
				)
				(pin bidirectional line
					(at 31.75 -69.85 180)
					(length 2.54)
					(name "DDBUS2")
					(number "50")
				)
				(pin bidirectional line
					(at 31.75 -72.39 180)
					(length 2.54)
					(name "DDBUS3")
					(number "51")
				)
				(pin bidirectional line
					(at 31.75 -74.93 180)
					(length 2.54)
					(name "DDBUS4")
					(number "52")
				)
				(pin bidirectional line
					(at 31.75 -77.47 180)
					(length 2.54)
					(name "DDBUS5")
					(number "53")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCCIO")
					(number "54")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "55")
				)
				(pin bidirectional line
					(at 31.75 -80.01 180)
					(length 2.54)
					(name "DDBUS6")
					(number "56")
				)
				(pin bidirectional line
					(at 31.75 -82.55 180)
					(length 2.54)
					(name "DDBUS7")
					(number "57")
				)
				(pin bidirectional line
					(at 31.75 -104.14 180)
					(length 2.54)
					(name "GPIO7")
					(number "58")
				)
				(pin bidirectional line
					(at 31.75 -91.44 180)
					(length 2.54)
					(name "GPIO2")
					(number "59")
				)
				(pin bidirectional line
					(at 31.75 -88.9 180)
					(length 2.54)
					(name "GPIO1")
					(number "60")
				)
				(pin bidirectional line
					(at 31.75 -86.36 180)
					(length 2.54)
					(name "GPIO0")
					(number "61")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VCC_USB")
					(number "62")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DM")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DP")
					(number "64")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 2.54)
					(name "REF")
					(number "65")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCC_PD")
					(number "66")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "PD1_CC2")
					(number "67")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "PD1_SVBUS")
					(number "68")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PD1_VCONN")
					(number "69")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "PD1_CC1")
					(number "70")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PD2_CC1")
					(number "71")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PD2_SVBUS")
					(number "72")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PD2_CC2")
					(number "73")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 2.54)
					(hide yes)
					(name "VCORE")
					(number "74")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 2.54)
					(name "~{PWREN}")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EECS")
					(number "76")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "77")
				)
			)
			(embedded_fonts no)
		)
)
