(footprint "Amphenol_G14A421211112HR"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 5.4 -5.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Amphenol_G14A421211112HR"
		(at 0 6.385 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.06)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.22 9.885 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.22 11.085 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.22 12.285 0)
		(layer "F.Fab")
	)
	(fp_text user "PCB EDGE"
		(at 2.8 2.95 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.42 -1.395 90)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.95 -1.395 90)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd roundrect
		(at -4.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A2" smd roundrect
		(at -4.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A3" smd roundrect
		(at -3.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A4" smd roundrect
		(at -3.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A5" smd roundrect
		(at -2.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A6" smd roundrect
		(at -2.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A7" smd roundrect
		(at -1.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A8" smd roundrect
		(at -1.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A9" smd roundrect
		(at -0.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A10" smd roundrect
		(at -0.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A11" smd roundrect
		(at 0.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A12" smd roundrect
		(at 0.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A13" smd roundrect
		(at 1.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A14" smd roundrect
		(at 1.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A15" smd roundrect
		(at 2.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A16" smd roundrect
		(at 2.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A17" smd roundrect
		(at 3.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A18" smd roundrect
		(at 3.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A19" smd roundrect
		(at 4.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A20" smd roundrect
		(at 4.75 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "A21" smd roundrect
		(at 5.25 -2.115 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B1" smd roundrect
		(at -5.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B2" smd roundrect
		(at -4.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B3" smd roundrect
		(at -4.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B4" smd roundrect
		(at -3.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B5" smd roundrect
		(at -3.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B6" smd roundrect
		(at -2.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B7" smd roundrect
		(at -2.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B8" smd roundrect
		(at -1.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B9" smd roundrect
		(at -1.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B10" smd roundrect
		(at -0.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B11" smd roundrect
		(at -0.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B12" smd roundrect
		(at 0.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B13" smd roundrect
		(at 0.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B14" smd roundrect
		(at 1.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B15" smd roundrect
		(at 1.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B16" smd roundrect
		(at 2.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B17" smd roundrect
		(at 2.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B18" smd roundrect
		(at 3.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B19" smd roundrect
		(at 3.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B20" smd roundrect
		(at 4.25 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "B21" smd roundrect
		(at 4.75 -4.305 90)
		(size 0.91 0.31)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
	)
	(pad "SH" smd roundrect
		(at -6.91 -3.915 90)
		(size 1.38 1.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at -6.91 0.805 90)
		(size 1.81 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 6.91 -3.915 90)
		(size 1.38 1.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 6.91 0.805 90)
		(size 1.81 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_g14a421211112hr.glb"
		(offset
			(xyz 0 -0.385 2.15)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "antmicro_g14a421211112hr.glb"
		(offset
			(xyz 0 -22.75 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -180 -0)
		)
	)
)
