(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "OCuLink_x4_Amphenol_G14A421211112HR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "OCuLink_x4_Amphenol_G14A421211112HR"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "OCuLink_x4_Amphenol_G14A421211112HR"
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/g14a421x1bxxxhr.pdf"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Connectors OCulink, Receptacle, 0.5mm pitch, 4X, R/A SMT with shell leg SMT type, 30U\" gold plating, LCP, black, T&R packing"
				(at 39.37 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "G14A421211112HR"
				(at 39.37 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONNECTOR, PCIE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "OCuLink_x4_Amphenol_G14A421211112HR_1_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "V_{ACT}_RX_3V3")
					(number "A1")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PER0+")
					(number "A3")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PER0-")
					(number "A4")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PER1+")
					(number "A6")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PER1-")
					(number "A7")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A8")
				)
				(pin no_connect line
					(at 21.59 -76.2 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "~{CWAKE}")
					(number "A10")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(name "GND")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VSP1")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VSP2")
					(number "A13")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A14")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PER2+")
					(number "A15")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PER2-")
					(number "A16")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A17")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PER3+")
					(number "A18")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PER3-")
					(number "A19")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A20")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "5V")
					(number "A21")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "5V")
					(number "B1")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PET0+")
					(number "B3")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PET0-")
					(number "B4")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PET1+")
					(number "B6")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PET1-")
					(number "B7")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SCL")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SDA")
					(number "B10")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "~{PERST}")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "~{CPRSNT}")
					(number "B13")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B14")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PET2+")
					(number "B15")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PET2-")
					(number "B16")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B17")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 3.81)
					(name "PET3+")
					(number "B18")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "PET3-")
					(number "B19")
				)
				(pin passive line
					(at 25.4 -91.44 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B20")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "V_{ACT}_TX_3V3")
					(number "B21")
				)
				(pin passive line
					(at 25.4 -88.9 180)
					(length 3.81)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
