(footprint "USB-A_Receptacle_Amphenol_GSB3112311HR"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Amphenol")
	(tags "Amphenol")
	(property "Reference" "REF**"
		(at 0 -7.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-A_Receptacle_Amphenol_GSB3112311HR"
		(at 0 14.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Edge of board"
		(at 12.8 13.6 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -4.6 16.3 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.6 17.501 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.6 18.7 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.499 0 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 4.498 0 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 6.999 0 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 7.499 -1.499 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.499 -1.499 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 3.499 -1.499 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 1.499 -1.499 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -0.5 -1.499 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 -3.2 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.499 -3.2 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 4.498 -3.2 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 6.999 -3.2 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 7.499 -4.7 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 5.499 -4.7 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 3.499 -4.7 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.499 -4.7 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at -0.5 -4.7 90)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -3.072 -3.68 90)
		(size 2.9 2.9)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -3.072 2 90)
		(size 2.9 2.9)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 10.07 -3.68 90)
		(size 2.9 2.9)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 10.169 2 90)
		(size 2.9 2.9)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_gsb3112311hr.glb"
		(offset
			(xyz 3.5 -3.4 12.6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "antmicro_gsb3112311hr.glb"
		(offset
			(xyz 3.5 -24 4.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "antmicro_gsb3112311hr.glb"
		(offset
			(xyz 3.5 -24 12.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
