(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-A_Amphenol_GSB3112311HR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 15.24 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-A_Amphenol_GSB3112311HR"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-A_Amphenol_GSB3112311HR"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/gsb311231hr.pdf"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB-A (USB TYPE-A) USB 3.2 Gen 1 (USB 3.1 Gen 1, Superspeed (USB 3.0)) Receptacle Connector 5 Position Through Hole, Right Angle"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GSB3112311HR"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "USB, CONNECTOR, THT, HORIZONTAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-A_Amphenol_GSB3112311HR_1_1"
				(text "PORT 1"
					(at -17.526 0 0)
				)
				(pin passive line
					(at 0 0 180)
					(length 2.54)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -6.35 180)
					(length 2.54)
					(name "D-")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -3.81 180)
					(length 2.54)
					(name "D+")
					(number "3")
				)
				(pin power_in line
					(at 0 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -11.43 180)
					(length 2.54)
					(name "SSRX-")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -8.89 180)
					(length 2.54)
					(name "SSRX+")
					(number "6")
				)
				(pin power_in line
					(at 0 -21.59 180)
					(length 2.54)
					(name "GND_DRAIN")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -16.51 180)
					(length 2.54)
					(name "SSTX-")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -13.97 180)
					(length 2.54)
					(name "SSTX+")
					(number "9")
				)
				(pin passive line
					(at 0 -24.13 180)
					(length 2.54)
					(name "SHIELD")
					(number "SH")
				)
			)
			(symbol "USB-A_Amphenol_GSB3112311HR_2_1"
				(text "PORT 2"
					(at -17.526 0 0)
				)
				(pin power_in line
					(at 0 0 180)
					(length 2.54)
					(name "VBUS")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -6.35 180)
					(length 2.54)
					(name "D-")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -3.81 180)
					(length 2.54)
					(name "D+")
					(number "12")
				)
				(pin power_in line
					(at 0 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -11.43 180)
					(length 2.54)
					(name "SSRX-")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -8.89 180)
					(length 2.54)
					(name "SSRX+")
					(number "15")
				)
				(pin power_in line
					(at 0 -21.59 180)
					(length 2.54)
					(name "GND_DRAIN")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -16.51 180)
					(length 2.54)
					(name "SSTX-")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -13.97 180)
					(length 2.54)
					(name "SSTX+")
					(number "18")
				)
			)
			(embedded_fonts no)
		)
)
