(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-A_Plug_Amphenol_GSB316441CEU_Vertical"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 16.51 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-A_Plug_Amphenol_GSB316441CEU_Vertical"
				(at 16.51 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-A_Plug_Amphenol_GSB316441CEU_Vertical"
				(at 16.51 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.tme.eu/Document/2364eac009853909846f3925a1a25f87/GSB316441CEU.PDF"
				(at 16.51 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB 3.2, Type A, Plug, Right Angle SMT, 9 Pins, Offset 0.95mm, 3.2mm Height, Shell Dip with Nickel Plating, 30μin Gold, Blue High Temperature Housing, Tape and Reel Packaging"
				(at 16.51 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 16.51 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GSB316441CEU"
				(at 16.51 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 16.51 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 16.51 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, CONNECTOR, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-A_Plug_Amphenol_GSB316441CEU_Vertical_1_1"
				(pin power_in line
					(at 0 0 180)
					(length 3.81)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -3.81 180)
					(length 3.81)
					(name "D-")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -6.35 180)
					(length 3.81)
					(name "D+")
					(number "3")
				)
				(pin power_in line
					(at 0 -30.48 180)
					(length 3.81)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 3.81)
					(name "STDA_SSRX-")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 3.81)
					(name "STDA_SSRX+")
					(number "6")
				)
				(pin power_in line
					(at 0 -22.86 180)
					(length 3.81)
					(name "GND_DRAIN")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -16.51 180)
					(length 3.81)
					(name "STDA_SSTX-")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -19.05 180)
					(length 3.81)
					(name "STDA_SSTX+")
					(number "9")
				)
				(pin passive line
					(at 0 -26.67 180)
					(length 3.81)
					(name "SHIELD")
					(number "SH1")
				)
				(pin passive line
					(at 0 -26.67 180)
					(length 3.81)
					(name "SHIELD")
					(number "SH2")
				)
			)
			(embedded_fonts no)
		)
)
