(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-A_Amphenol_GSB4112312HR"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 28.575 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-A_Amphenol_GSB4112312HR"
				(at 27.94 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-A_Amphenol_GSB4112312HR"
				(at 27.94 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/documentation/datasheet/inputoutput/io_usb_3_1_gen2_gsb4x.pdf"
				(at 27.94 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB 3.2 GEN 2, Type A, Receptacle, Right Angle Stacked, 18 Pins, Shell with Nickel Plating, 30μin Gold, Dip 2.4mm, Blue High Temperature Housing, Tray Packaging"
				(at 28.575 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 27.94 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GSB4112312HR"
				(at 27.94 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, CONNECTOR, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-A_Amphenol_GSB4112312HR_0_0")
			(symbol "USB-A_Amphenol_GSB4112312HR_0_1")
			(symbol "USB-A_Amphenol_GSB4112312HR_1_0"
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "D-_1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "D+_1")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SSRX-_1")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SSRX+_1")
					(number "6")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 2.54)
					(name "GND_DRAIN_1")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "SSTX-_1")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SSTX+_1")
					(number "9")
				)
			)
			(symbol "USB-A_Amphenol_GSB4112312HR_1_1"
				(text "PORT 1"
					(at 21.59 -1.27 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBUS_1")
					(number "1")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 2.54)
					(name "GND_1")
					(number "4")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "SHIELD")
					(number "SH")
				)
			)
			(symbol "USB-A_Amphenol_GSB4112312HR_2_0"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D-_2")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D+_2")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SSRX-_2")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SSRX+_2")
					(number "15")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND_DRAIN_2")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SSTX-_2")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SSTX+_2")
					(number "18")
				)
			)
			(symbol "USB-A_Amphenol_GSB4112312HR_2_1"
				(text "PORT 2"
					(at 21.59 -1.27 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBUS_2")
					(number "10")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 2.54)
					(name "GND_2")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
