(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "HD3SS3220IRNHR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "HD3SS3220IRNHR"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "HD3SS3220IRNHR"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/hd3ss3220.pdf?ts=1663000043694&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC 10-Gbps USB 3.1 Type-C 2:1 mux with DRP Controller 30-WQFN -40°C to 85°C"
				(at 41.91 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "HD3SS3220IRNHR"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, INTERFACE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "HD3SS3220IRNHR_1_1"
				(pin passive line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "CC2")
					(number "1")
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "CC1")
					(number "2")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CURRENT_MODE")
					(number "3")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PORT")
					(number "4")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "VBUS_DET")
					(number "5")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "TX+")
					(number "6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "TX-")
					(number "7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC33")
					(number "8")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RX+")
					(number "9")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RX-")
					(number "10")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(name "DIR")
					(number "11")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ENn_MUX")
					(number "12")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin passive line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "RX1-")
					(number "14")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "RX1+")
					(number "15")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "TX1-")
					(number "16")
				)
				(pin passive line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "TX1+")
					(number "17")
				)
				(pin passive line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "RX2-")
					(number "18")
				)
				(pin passive line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "RX2+")
					(number "19")
				)
				(pin passive line
					(at 27.94 -58.42 180)
					(length 2.54)
					(name "TX2-")
					(number "20")
				)
				(pin passive line
					(at 27.94 -60.96 180)
					(length 2.54)
					(name "TX2+")
					(number "21")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "ADDR")
					(number "22")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "INT_N/OUT3")
					(number "23")
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "VCONN_FAULT_N")
					(number "24")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "SDA/OUT1")
					(number "25")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "SCL/OUT2")
					(number "26")
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "ID")
					(number "27")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "ENn_CC")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD5")
					(number "30")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
			)
			(embedded_fonts no)
		)
)
