(footprint "HDMI-A_Plug_Adam_Tech_HDMI-PLUG-OM3"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.01 9.69 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI-A_Plug_Adam_Tech_HDMI-PLUG-OM3"
		(at 0.01 11.11 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Pcb_Edge"
		(at -1.2 4.81 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -8.24 13.11 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.24 14.31 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.24 15.51 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 4.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 4 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" smd rect
		(at 3.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at 3 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" smd rect
		(at 2.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at 2 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" smd rect
		(at 1.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at 1 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" smd rect
		(at 0.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 0 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" smd rect
		(at -0.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -1 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" smd rect
		(at -1.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at -2 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" smd rect
		(at -2.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at -3 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" smd rect
		(at -3.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at -4 7.19 180)
		(size 0.7 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" smd rect
		(at -4.5 7.19 180)
		(size 0.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "SH" smd rect
		(at -6.69 7.18)
		(size 1.6 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "SH" smd rect
		(at -6.69 7.18)
		(size 1.6 3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "SH" smd rect
		(at 6.71 7.18)
		(size 1.6 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "SH" smd rect
		(at 6.71 7.18)
		(size 1.6 3)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_hdmi_plug_om3.glb"
		(offset
			(xyz 0 1.2 -0.9)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
