(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_RJ45_JTH-0024NL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_RJ45_JTH-0024NL"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_RJ45_JTH-0024NL"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/447/JTH_0024NL-3072047.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular Connectors / Ethernet Connectors 1X1 TAB DOWN W/LED'S ETHERNET (NON PoE)"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "JTH-0024NL"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Pulse Electronics"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RJ45, HORIZONTAL, THT, ETHERNET, CONNECTOR, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "CONN18_5-2337992-8_TEC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_RJ45_JTH-0024NL_1_1"
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "CT3")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "T2-")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "T2+")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "T3+")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "T3-")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "CT2")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "CT4")
					(number "7")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "T1+")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "T1-")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "T4-")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "T4+")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "CT1")
					(number "12")
				)
				(pin passive line
					(at 21.59 -30.48 180)
					(length 2.54)
					(name "LED_GRN-")
					(number "13")
				)
				(pin passive line
					(at 21.59 -27.94 180)
					(length 2.54)
					(name "LED_GRN+")
					(number "14")
				)
				(pin passive line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "LED_YG_Y-")
					(number "15")
				)
				(pin passive line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "LED_COM+")
					(number "16")
				)
				(pin passive line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "LED_YG_G-")
					(number "17")
				)
				(pin passive line
					(at 21.59 -35.56 180)
					(length 2.54)
					(name "SHIELD")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
